# Requirements Specification

This document captures JellyTau's user requirements, software requirements,
traceability matrix, test traceability, and known technical debt.

For a narrative overview of the system design, see
[docs/architecture/](architecture/). For development workflows, see the
[README](../README.md) and [scripts/README.md](../scripts/README.md).

## 1. User Requirements

| ID | Requirement | Priority | Status |
|----|-------------|----------|--------|
| UR-001 | Run the app on multiple platforms (Linux, Android) | High | In Progress |
| UR-002 | Access media when online or offline | High | Done |
| UR-003 | Play videos | High | Done |
| UR-004 | Play audio uninterrupted | High | Done |
| UR-005 | Control media playback (pause, play, skip, scrub) | High | Done |
| UR-006 | Control media when device is on lock screen or via BLE headsets | Medium | Done |
| UR-007 | Navigate media in library | High | Done |
| UR-008 | Search media across libraries | High | Done |
| UR-009 | Connect to Jellyfin to access media | High | Done |
| UR-010 | Control playback of Jellyfin remote sessions | Low | Done |
| UR-011 | Download media on demand | Medium | Done |
| UR-012 | Login info shall be stored securely and persistently | High | Done |
| UR-013 | View and manage downloaded media | Medium | Done |
| UR-014 | Make and edit playlists of music that sync back to Jellyfin | Medium | Done |
| UR-015 | View and manage current audio queue (add, reorder tracks) | Medium | Done |
| UR-016 | Change system settings while playing (brightness, volume) | Low | Planned |
| UR-017 | Like or unlike audio, albums, movies, etc. | Medium | Done |
| UR-018 | Choose to download series, albums, songs, artist discography | Medium | Done |
| UR-019 | Resume playback from where you left off (movies, shows, albums) | High | Done |
| UR-020 | Select subtitles for video content | High | Done |
| UR-021 | Select audio track for video content | High | Done |
| UR-022 | Control streaming quality and transcoding settings | Medium | Planned |
| UR-023 | View "Next Up" / Continue Watching on home screen; auto-play next episode with countdown popup and configurable episode limit | Medium | Done |
| UR-024 | View recently added content on server | Medium | Done |
| UR-025 | Sync watch history and progress back to Jellyfin | High | Done |
| UR-026 | Sleep timer for audio and video playback (roller UI, time/track/episode modes) | Low | Done |
| UR-027 | Audio equalizer for sound customization | Low | Done (Linux only) |
| UR-028 | Navigate to artist/album by tapping names in now playing view | High | Done |
| UR-029 | Toggle between grid and list view in library | Medium | Done |
| UR-030 | Quick genre browsing and filtering | Medium | Done |
| UR-031 | Crossfade between audio tracks | Low | Not implemented (blocked — see DR-034) |
| UR-032 | Gapless playback for seamless album listening | Medium | Done (Linux only) |
| UR-033 | Volume normalization to prevent volume jumps between tracks | Low | Done (Linux only) |
| UR-034 | Rich home screen with hero banners, carousels, and personalized sections | High | Done |
| UR-035 | View cast/crew (actors, directors) on movie/show detail pages | High | Done |
| UR-036 | Navigate to actor/person page showing their filmography | Medium | Done |
| UR-037 | Visually appealing video library with poster grids and metadata | High | Done |
| UR-038 | Movie/show detail page with backdrop, ratings, and rich metadata | High | Done |
| UR-039 | Navigate between main sections via bottom navigation bar | High | Done |
| UR-040 | Keep a video's audio playing when the app is backgrounded or the screen is locked, stopping video decode until the app returns to the foreground (per-player toggle; Android) | Medium | Done (pending device verification) |
| UR-041 | Continue watching *locally-playing video* in a floating picture-in-picture window when leaving the app (Android) — PiP applies to video only, never to audio playback, library/menu browsing, or remote/cast sessions | Medium | Done |
| UR-042 | Authenticate to a server and manage the session lifecycle (connect, log in, Quick Connect, background session verification, re-authenticate, log out) | High | Done |
| UR-043 | Automatically detect server reachability and switch between online and offline operation without user intervention | High | Done |
| UR-044 | Pin downloaded media so it is protected from automatic cache eviction | Low | Done |
| UR-045 | Predictively pre-cache likely-next media (queue lookahead and album affinity) within a storage budget | Low | Done |
| UR-046 | Group multiple remote players into a synchronized playback group (LMS SyncGroups) | Low | Done |
| UR-047 | Manage multiple Jellyfin servers (add, list, remove) and switch the active server/account | Medium | Planned (backend store done; switcher UI pending) |
| UR-048 | See the next episodes of a series directly below the episode/series being viewed, above cast and similar-shows content, so continuing a show is the shortest path (see [ux-flows.md §5B](ux-flows.md)) | High | Done |
| UR-049 | Search is scoped by where it was started — inside a library it searches that library, from Home/library-root/search-tab it searches everything — with the scope shown as filter chips under the search bar that preselect from context and can be changed without retyping (see [ux-flows.md §6.1](ux-flows.md)) | High | Implemented |
| UR-050 | Reorder search result groups (Songs, Albums, Artists, Movies, TV Shows) by drag and drop in settings, so the media a user cares about most appears first (see [ux-flows.md §6.3](ux-flows.md)) | Medium | Implemented |
| UR-051 | Browse library pages in a consistent layout where card shape signals media type (square music, poster video, thumbnail episode), ordinal content stays listed, and the grid/list preference persists across pages (see [ux-flows.md §5A](ux-flows.md)) | Medium | Partial (implemented; toggle not reachable from settings) |
| UR-052 | While offline, library pages show only media available on the device by default, with an opt-in toggle that additionally reveals the cached server catalog as greyed-out entries which can be queued for download on the next reconnect | High | Done |
| UR-053 | Restrict media downloads to unmetered networks via a "WiFi Only" setting: when enabled, queued downloads are held while the device is on cellular or a metered connection (including metered WiFi hotspots) and resume automatically once an unmetered network is available | Medium | Done (pending device verification) |
| UR-054 | Reach account actions (Settings, Downloads, Display preferences, Sign out) from every authenticated screen via a single account menu anchored to the user's name, identical on desktop and mobile (see [ux-flows.md §1.2](ux-flows.md)) | High | Done |
| UR-055 | Browse downloaded media as an offline-scoped library — reusing the same library grids, cards, and detail pages as online browsing, showing only libraries/containers with downloaded content — with the transfer-progress list demoted to a secondary "Transfers" view (see [ux-flows.md §7.2](ux-flows.md)) | High | Done |
| UR-056 | See how much disk each downloaded item/album/series consumes, in familiar rounded units shown on the card and detail page, with a device total on the Downloaded surface and a reclaim amount stated at the point of removal (see [ux-flows.md §7.3.1](ux-flows.md)) | Medium | Done |
| UR-057 | Settings apply the instant a control is changed — no "Save" button and no save/dirty state — so leaving the page never loses a change; sliders show a live readout while dragging but persist on release (see [ux-flows.md §8.1](ux-flows.md)) | Medium | Done |
| UR-058 | On the home screen, a tap on a media card opens the item (movie/episode detail page, or the series Episode Focus View for episodes) rather than starting playback; a long-press starts "play now" after a confirm; an episode detail/focus page links back to its parent series and season (see [ux-flows.md §5B.5](ux-flows.md) and [§5B.1](ux-flows.md)) | Medium | Done |
| UR-059 | Skipping to the next episode records the episode left behind as **fully watched** rather than saving a mid-episode resume point — skipping means "done with this one", not "stopped here" — and Continue Watching hides episodes the viewer has already moved past (a partial position behind that series' next-up episode), so the row only ever offers genuinely unfinished media | Medium | Done |
| UR-060 | Search results are ordered by how well they match: a name that *starts* with the query outranks one matching mid-word (typing "parks" finds "Parks and Recreation" before "Sparks of Love"), and at equal match quality a container outranks its contents (a series before its episodes). Results are grouped into distinct categories — TV Shows, Episodes, Movies, Songs, Albums, Artists and People — so a show never competes with its own episodes for the same slot, and searching an actor's name reaches their bio | High | Done |
| UR-061 | Double tapping the video skips within it — right half jumps **forward 30 seconds**, left half jumps **back 10 seconds** — with an on-screen indicator naming the amount. A double tap leaves the play state unchanged — playing jumps and keeps playing, paused jumps and stays paused — because the second tap re-toggles what the first tap toggled (see DR-098); the skip lands relative to the position the player actually reports, and repeated double taps accumulate rather than all skipping from the same spot | Medium | Done |
| UR-062 | Opening a TV series lands the viewer **where they are in it**, not at season 1: the series page scrolls the current season into view and highlights the current episode, and the hero button opens that episode (labelled `Resume S2E4` / `Play S1E1`). "Current" means the episode in progress, else the server's Next Up for that series, else the first unwatched episode, else the first — resolved by the backend so it also works offline. A season is **never a page of its own**: every route that names a season lands on the series with that season in view, so the episodes of all seasons are always one continuous scrollable list | High | Done |
| UR-063 | Each video library is **one page**, not three. Browsing (hero, Continue Watching, Next Up, Recently Added, genre rows), the full title grid, and the genre browser are tabs of `/library/tv` and `/library/movies` rather than separate routes with inconsistent names (`/library/tv/shows` vs `/library/movies/all`, `/library/shows/genres` vs `/library/movies/genres`). The old routes redirect so existing links keep working | Medium | Done |
| UR-064 | Watch history can be **erased**, per series and per season, from the series page. Clearing marks every episode inside unwatched and clears resume positions, so the show returns to "never watched" and reopens on its premiere. It asks for confirmation first (it cannot be undone) and requires a connection to the server, since history cleared only locally would be undone by the next sync | Medium | Done |
| UR-065 | Search answers from a **locally indexed copy of the library**, so results appear as fast as the device can query rather than at the speed of a round trip to the server, and the same results are found with the server unreachable. A background job keeps the index current — refreshing on a schedule rather than only at app start, dropping media removed from the server, and covering everything the result groups can show (including artists and people). The server is still queried in the background so media added since the last index still turns up, merged in without reordering what is already on screen | High | Implemented |
| UR-066 | The app's own chrome stays clear of the device's system chrome. On Android the bottom navigation sits above the navigation/gesture bar instead of underneath it, the header clears the status bar, and full-screen video and audio playback keep their controls inside the usable screen — clear of the gesture bar and, in landscape, of the display notch. This must hold across navigation modes (gesture and 3-button) and rotation, not only on the handsets it happened to be tested on | High | Done |
| UR-067 | Favourited media can be **found again**. A Favourites page lists everything favourited across all libraries, scoped by tabs (All / Movies / Shows / Music); the home screen carries favourite rows for movies, shows and music, hidden when a category is empty; and each library page can be filtered to favourites in place. Without this the like button writes to a store nothing reads | Medium | Done |
| UR-068 | Anything the app shows can be favourited where it is shown — from a movie, series, episode, album, artist or playlist page, and from any card in a grid or carousel — not only from the player while the item happens to be playing | Medium | Done |
| UR-069 | Favourite state agrees with the server in both directions. An item favourited in another Jellyfin client shows as favourited here without being touched, and an item favourited here while the server is unreachable reaches the server once it returns — without the user going back to the screen where they marked it | Medium | Done |
| UR-070 | Playback quality is the viewer's choice: the player offers the bitrates the server can produce for what is playing, and changing one resumes at the same point with the same audio and subtitle tracks. Because the chosen rendition can change at any moment, nothing that streams for playback is treated as a stored copy unless it happens to be byte-identical to the real file | Medium | Proposed |
| UR-071 | Media the viewer is watching can be **kept**, by a whole-file download that runs in the background independently of playback and at its own quality, so it is unaffected by bitrate changes. Where the streamed bytes already are that file (direct play), they are kept rather than fetched twice. A completed download is then played from disk rather than streamed again | Medium | Proposed |

---

## 2. Software Requirements

### 2.1 Integration Requirements

External system integrations and platform-specific implementations.

| ID | Requirement | Category | Traces To | Status |
|----|-------------|----------|-----------|--------|
| IR-001 | Build system supporting multiple targets (Linux, Android) | Build | UR-001 | Done |
| IR-002 | Build scripts for Android and Linux | Build | UR-001 | Done |
| IR-003 | Integration of libmpv for Linux playback | Playback | UR-003, UR-004 | Done |
| IR-004 | Integration of ExoPlayer for Android playback | Playback | UR-003, UR-004 | In Progress (basic playback works, audio settings missing) |
| IR-005 | MPRIS D-Bus integration for Linux lockscreen/media controls | Platform | UR-006 | Planned |
| IR-006 | Android MediaSession integration for lockscreen controls | Platform | UR-006 | Done |
| IR-007 | Bluetooth AVRCP integration via system media session | Platform | UR-006 | Planned |
| IR-008 | Android audio focus handling (pause on call) | Platform | UR-004, UR-006 | Done |
| IR-009 | Jellyfin API client for authentication | API | UR-009, UR-012 | Done |
| IR-010 | Jellyfin API client for library browsing | API | UR-007, UR-008 | Done |
| IR-011 | Jellyfin API client for playback streaming | API | UR-003, UR-004 | Done |
| IR-012 | Jellyfin Sessions API for remote playback control | API | UR-010 | Done |
| IR-021 | Android MediaRouter integration for remote volume in system panel | Platform | UR-010, UR-016 | Planned |
| IR-013 | SQLite integration for local database | Storage | UR-002, UR-011 | Done |
| IR-014 | Secure credential storage (keyring/keychain) | Security | UR-012 | Done |
| IR-015 | Jellyfin API client for playback progress reporting | API | UR-019, UR-025 | Done |
| IR-016 | Jellyfin API client for subtitle/audio track info | API | UR-020, UR-021 | Done |
| IR-017 | Jellyfin API client for transcoding parameters | API | UR-022 | Planned |
| IR-018 | libmpv subtitle rendering and selection | Playback | UR-020 | Planned |
| IR-019 | libmpv audio track selection | Playback | UR-021 | Planned |
| IR-020 | libmpv/ExoPlayer equalizer integration | Playback | UR-027 | Done (Linux/MPV; Android parity pending) |
| IR-022 | Jellyfin API client for person/cast data | API | UR-035, UR-036 | Done |
| IR-023 | Database schema for person/cast caching | Storage | UR-035, UR-036 | Done |
| IR-024 | Jellyfin API client for home screen data (featured, continue watching) | API | UR-034 | Done |
| IR-025 | Android background-audio handoff: WebView `<video>` → native ExoPlayer foreground service on background/lock, and back on foreground (audio continues, video decode stops) | Platform | UR-040 | Done (pending device verification) |
| IR-026 | Android picture-in-picture: auto-enter on user-leave-hint via `enterPictureInPictureMode`, **only while a local video surface is actively rendering** (never for audio-only playback, menu/library browsing, or remote/cast sessions — enforced by the native `canEnterPip` guard, re-checked at leave time); aspect-ratio sizing; a play/pause RemoteAction that **reflects live player play/pause state** (updated whenever playback state changes, not only on button press); WebView hide/restore on mode change | Platform | UR-041 | Done |
| IR-027 | Jellyfin `/System/Info/Public` reachability probe used as an offline→online recovery detector | API | UR-043 | Done |
| IR-028 | Jellyfin/LMS SyncGroups API client (list, create, join, unsync, dissolve sync groups) | API | UR-046 | Done |
| IR-029 | Android `ConnectivityManager`/`NetworkCapabilities` transport probe with a `NetworkCallback` change subscription, surfaced to the frontend via the `AndroidNetworkType` JS bridge and the `jellytau-network-changed` WebView event (requires `ACCESS_NETWORK_STATE`) | Platform | UR-053 | Done (pending device verification) |
| IR-030 | Scheduled full-catalog crawl of every library (`Recursive=true`, paged) feeding the local index, driven by a Rust background task and the `ConnectivityMonitor` reconnect signal rather than by the frontend | Storage | UR-065 | Implemented |
| IR-031 | Android `WindowInsets` bridge: an `OnApplyWindowInsetsListener` on the decor view reports `systemBars() | displayCutout()` in CSS pixels, pushed into the WebView as `jt-inset` CSS custom properties plus a `jellytau-insets-changed` event, and pullable via the `AndroidInsets` JS bridge | Platform | UR-066 | Done (pending device verification) |
| IR-032 | Whole-file background download of the item being played, reusing the existing resumable download worker and the Range-capable `/Videos/{id}/stream.mp4` endpoint; plus per-platform read-through caching hooks (ExoPlayer `CacheDataSource`, mpv `stream-record`) for direct-play sessions only | Storage | UR-071 | Proposed |

### 2.2 Jellyfin API Requirements

API endpoints and data contracts required for Jellyfin integration.

| ID | Requirement | Endpoint Category | Traces To | Status |
|----|-------------|-------------------|-----------|--------|
| JA-001 | Server connection and discovery | System | UR-009 | Done |
| JA-002 | User authentication (username/password) | Users | UR-009, UR-012 | Done |
| JA-003 | Get user library views | UserViews | UR-007 | Done |
| JA-004 | Get library items (paginated) | Items | UR-007 | Done |
| JA-005 | Get item details and metadata | Items | UR-007 | Done |
| JA-006 | Search across libraries | Items | UR-008 | Done |
| JA-007 | Get playback info and stream URL | MediaInfo | UR-003, UR-004 | Done |
| JA-008 | Get available subtitles for item | MediaInfo | UR-020 | Done |
| JA-009 | Get available audio tracks for item | MediaInfo | UR-021 | Done |
| JA-010 | Report playback start | Sessions | UR-025 | Done |
| JA-011 | Report playback progress (periodic) | Sessions | UR-025 | Done |
| JA-012 | Report playback stopped | Sessions | UR-025 | Done |
| JA-013 | Get resume position for item | UserData | UR-019 | Done |
| JA-014 | Get "Next Up" items | Shows | UR-023 | Done |
| JA-015 | Get "Continue Watching" items | Items | UR-023 | Done |
| JA-016 | Get recently added items | Items | UR-024 | Done |
| JA-017 | Mark item as favorite | UserData | UR-017 | Done |
| JA-018 | Remove item from favorites | UserData | UR-017 | Done |
| JA-019 | Get/create/update playlists | Playlists | UR-014 | Done |
| JA-020 | Add/remove items from playlist | Playlists | UR-014 | Done |
| JA-021 | Get active sessions list | Sessions | UR-010 | Done |
| JA-022 | Send playback commands to remote session (play/pause/stop) | Sessions | UR-010 | Done |
| JA-023 | Send seek command to remote session | Sessions | UR-010 | Done |
| JA-024 | Send next/previous track commands to remote session | Sessions | UR-010 | Done |
| JA-025 | Play specific item on remote session | Sessions | UR-010 | Done |
| JA-026 | Send volume/mute commands to remote session | Sessions | UR-010 | Done |
| JA-027 | Get transcoding options | MediaInfo | UR-022 | Planned |
| JA-028 | Get image/artwork URLs | Images | UR-007 | Done |
| JA-029 | Get cast/crew for item (actors, directors) | Items | UR-035 | Done |
| JA-030 | Get person details and filmography | Persons | UR-036 | Done |
| JA-031 | Get items by person (actor/director filmography) | Items | UR-036 | Done |
| JA-032 | Get audio-only stream URL for a video item (selected audio-stream index) | MediaInfo | UR-040 | Done |
| JA-033 | Query favourite items (`Filters=IsFavorite`, recursive, scoped by item type) | Items | UR-067 | Done |
| JA-034 | Read `UserData` (favourite, played, resume position) from item responses | UserData | UR-069 | Done |
| JA-035 | Mark item played (`POST /Users/{userId}/PlayedItems/{itemId}`) | UserData | UR-025 | Done |

### 2.3 Development Requirements

Internal architecture, components, and application logic.

| ID | Requirement | Category | Traces To | Status |
|----|-------------|----------|-----------|--------|
| DR-001 | Player state machine (idle, loading, playing, paused, seeking, error) | Player | UR-005 | Done |
| DR-002 | MediaItem struct tracking source, location, duration, metadata | Player | UR-003, UR-004 | Done |
| DR-003 | Source-agnostic media abstraction (Remote, Local, DirectUrl) | Player | UR-002, UR-011 | Done |
| DR-004 | PlayerBackend trait for platform-agnostic playback | Player | UR-003, UR-004 | Done |
| DR-005 | Queue manager with shuffle, repeat, history | Player | UR-005, UR-015 | Done |
| DR-006 | Audio pre-caching for seamless track transitions | Player | UR-004 | Planned |
| DR-007 | Library browsing screens (grid view, search, filters) | UI | UR-007, UR-008 | Done |
| DR-008 | Album/Series detail view with track listing | UI | UR-007 | Done |
| DR-009 | Audio player UI (mini player, full screen) | UI | UR-005 | Done |
| DR-010 | Video player UI (fullscreen, controls overlay) | UI | UR-003, UR-005 | Done |
| DR-011 | Search bar with cross-library search | UI | UR-008 | Done |
| DR-012 | Local database for media metadata cache | Storage | UR-002 | Done |
| DR-013 | Repository pattern for online/offline data access | Storage | UR-002 | Done |
| DR-014 | Offline mutation queue for sync-back operations | Storage | UR-002, UR-014, UR-017 | Done |
| DR-015 | Download manager with queue and progress tracking | Storage | UR-011, UR-018 | Done |
| DR-016 | Thumbnail caching and sync with server | Storage | UR-007 | Done |
| DR-017 | "Manage Downloads" screen for local media management | UI | UR-013 | Done |
| DR-018 | Download buttons on library/album/player screens | UI | UR-011, UR-018 | Done |
| DR-019 | Playlist creation and editing UI | UI | UR-014 | Done |
| DR-020 | Queue management UI (add, remove, reorder) | UI | UR-015 | Done |
| DR-021 | Like/favorite functionality on media items | UI | UR-017 | Done |
| DR-022 | Resume position tracking and restoration on play | Player | UR-019 | Done |
| DR-023 | Subtitle selection UI in video player | UI | UR-020 | Done |
| DR-024 | Audio track selection UI in video player | UI | UR-021 | Done |
| DR-025 | Quality/transcoding settings UI | UI | UR-022 | Planned |
| DR-026 | "Continue Watching" / "Next Up" home section | UI | UR-023 | Done |
| DR-027 | "Recently Added" home section | UI | UR-024 | Done |
| DR-028 | Playback progress sync service (periodic reporting) | Player | UR-025 | Done |
| DR-029 | Sleep timer with roller UI, time/track/episode modes, and auto-stop (audio + video players) | Player | UR-026 | Done |
| DR-049 | Auto-play episode limit (configurable max episodes per session) | Player | UR-023 | Done |
| DR-050 | Reusable scroll picker (roller) component | UI | UR-026 | Done |
| DR-030 | Equalizer UI with presets and custom bands | UI | UR-027 | Done |
| DR-031 | Clickable artist/album links in now playing view | UI | UR-028 | Done |
| DR-032 | List view option for library browsing (albums, artists) | UI | UR-029 | Done |
| DR-033 | Genre browsing screen with quick filters | UI | UR-030 | Done |
| DR-034 | Crossfade engine with configurable duration (0-12s) | Player | UR-031 | Not implemented (blocked on MPV: single-stream audio chain; `acrossfade` needs 2 inputs — see docs/specs/playback-backend-unification.md) |
| DR-035 | Gapless playback between sequential tracks | Player | UR-032 | Done (Linux only) |
| DR-036 | Volume normalization with preset levels (Loud/Normal/Quiet) | Player | UR-033 | Done (Linux only) |
| DR-037 | Remote session browser and control UI | UI | UR-010 | Done |
| DR-038 | Home screen with hero banner carousel (featured/continue watching) | UI | UR-034 | Done |
| DR-039 | Home screen horizontal carousels (recently added, recommendations) | UI | UR-034, UR-024 | Done |
| DR-040 | Cast/crew section on movie/show detail pages | UI | UR-035 | Done |
| DR-041 | Person/actor detail page with filmography grid | UI | UR-036 | Done |
| DR-042 | Video library grid with poster cards, year, and rating badges | UI | UR-037 | Done |
| DR-043 | Movie/show detail page with backdrop hero, synopsis, and metadata | UI | UR-038 | Done |
| DR-044 | Horizontal scrolling actor/cast row with profile images | UI | UR-035 | Done |
| DR-045 | Bottom navigation bar with Home, Library, Search buttons | UI | UR-039 | Done |
| DR-046 | Dedicated search page with input and results | UI | UR-039 | Done |
| DR-047 | Next episode auto-play popup with configurable countdown and episode limit | Player | UR-023 | Done |
| DR-048 | Video settings (auto-play toggle, countdown duration, episode limit) | Settings | UR-023, UR-026 | Done |
| DR-051 | Background-audio toggle button in the video player controls (suppresses auto-PiP while enabled) | UI | UR-040 | Done (pending device verification) |
| DR-052 | Background-audio handoff state machine: on background/lock tear down the WebView `<video>`/HLS decode and start native audio-only playback at the current position; on foreground return position and resume `<video>`; exactly one audio source active at every transition (no dual audio) | Player | UR-040 | Done (pending device verification) |
| DR-053 | PictureInPictureManager: `canEnterPip` gate (local video surface actively rendering — false for audio, browsing, and remote/cast), aspect-ratio clamp, a RemoteAction play/pause receiver whose icon reflects live player state (refreshed on every playback-state change while in PiP, not only on button press), WebView hide/restore, surface re-fit on exit; plus the `AndroidPictureInPicture` JS bridge and the PiP button (shown only when PiP is supported) in the video player | UI | UR-041 | Done |
| DR-054 | Auth manager and session lifecycle: connect-to-server, login, Quick Connect verification poll (start/stop), session get/set, background session verifier, re-authenticate, logout | Auth | UR-042 | Done |
| DR-055 | ConnectivityMonitor deriving reachability from real repository traffic, with online/offline state, mark-reachable/unreachable reporting, and a probe-based recovery poller active only while offline | Connectivity | UR-043 | Done |
| DR-056 | Download pinning (pin/unpin/is-pinned) that excludes an item from smart-cache eviction | Storage | UR-044 | Done |
| DR-057 | Smart cache manager: album-affinity tracking, queue-lookahead pre-cache, storage-limit enforcement, config, stats, and recommendations | Storage | UR-045 | Done |
| DR-058 | Remote sync-group control (LMS SyncGroups): list, create, unsync a player, dissolve a group | Player | UR-046 | Done |
| DR-059 | Playback-mode transfer state machine: get/set current mode, transferring guard, transfer-to-remote / transfer-to-local, remote session status | Player | UR-010 | Done |
| DR-060 | Multi-server store and active-account selection: save/get/delete server, save/get user, set/get active user (per-server), active-session resolution | Storage | UR-047 | Partial (store done; server-switcher UI pending) |
| DR-061 | Episode Focus View: episode hero followed *immediately* by the "More Episodes" strip — a forward-biased window (~3 before / ~6 after) around the current episode, spanning season boundaries in series order, with the current episode present and badged, per-card resume progress and watched state, and click-to-swap focus (no playback) | UI | UR-048 | Done |
| DR-062 | Detail-page section ordering: continuation content precedes discovery content — Episode Focus View renders hero → episode strip → cast → similar; Series renders hero → seasons/episodes → cast → similar | UI | UR-048 | Done |
| DR-063 | Search scope taxonomy owned by Rust: `SearchScope` (All / Music / Movies / TV) crosses IPC as an opaque enum and `SearchScope::item_types()` expands it to Jellyfin item types, resolved once in `repository_search` before the cache and server paths diverge so online and offline filter identically; `All` expands to *no* filter rather than the union of the other scopes (which would drop People and folders). The frontend maps the originating route to a scope (`resolveSearchScope`, presentation) and never names an item type for search | Backend | UR-049 | Implemented |
| DR-064 | Scope chip row rendered under the search bar on both the search page and the in-library header search: preselected from context, horizontally scrollable, re-runs the search preserving the query on change | UI | UR-049 | Implemented |
| DR-065 | Thread `SearchOptions.includeItemTypes` through `library.search()` so the global/header search honours scope (backend online + offline paths already support it) | UI | UR-049 | Implemented |
| DR-066 | Persisted search result group order with a drag-and-drop settings list, keyboard-accessible reordering, a shipped default (see DR-091 for the current group set and order), and empty-group omission | Settings | UR-050 | Implemented |
| DR-067 | `SearchResults` renders groups in the user-configured order rather than hardcoded markup order, without altering intra-group ranking | UI | UR-050 | Implemented |
| DR-068 | Library card shape by media type: 1:1 square for music (circular mask for artists), 2:3 poster for movies/series/seasons, 16:9 for episodes and collection folders | UI | UR-051 | Done |
| DR-069 | Responsive library grid (2/3/4/5/6 columns across base→xl) with two-line truncated card text and artwork-overlay progress/watched state | UI | UR-051 | Done |
| DR-070 | Global persisted grid/list view preference honoured by browse pages, suppressed for ordinal content (album tracks, season episodes) | UI | UR-051, UR-029 | Partial (persisted store + page-header toggle; no settings entry) |
| DR-075 | Shared `AccountMenu` component: identity header (user + server), Downloads / Settings / Display entries, divider, Sign out last; anchored to the username/avatar trigger and identical on desktop and mobile | UI | UR-054 | Done |
| DR-076 | App shell exposes the header (and therefore the account menu) on every authenticated non-immersive route, including `/`, `/search`, and `/downloads`; only `/player/*` and `/login` remain chrome-free | UI | UR-054 | Done |
| DR-077 | Display section in Settings binding the existing persisted grid/list `viewMode` store, giving the preference a discoverable home | Settings | UR-054, UR-029 | Done |
| DR-078 | Catalog-visibility gate spanning the "Show all server media" toggle → `set_show_server_catalog` → `INCLUDE_CATALOG_BROWSE` → the synced-catalog UNION branch of offline `get_items`. Visibility resolves to `serverReachable \|\| showServerCatalog`, so offline with the toggle off lists downloaded/local media only | Storage | UR-052, UR-002 | Done |
| DR-079 | `isConnected` derives from backend-reported server reachability alone; `navigator.onLine` is advisory and may only trigger a recheck, never force or clear the offline state (a reachable LAN server while the browser reports offline, and an unreachable server on a live link, must both resolve correctly) | Connectivity | UR-052, UR-043 | Done |
| DR-080 | With the catalog-browse gate off, an empty offline `get_items` result is authoritative "no downloads here" and must be returned as-is; the hybrid repository must not treat it as a cache miss and fall through to the server | Storage | UR-052, UR-013 | Done |
| DR-074 | WiFi-only download gate: `NetworkState`/`NetworkType` transport model reported from the platform via `set_network_state`, checked in `pump_download_queue` before starting any pending row (cellular/metered/unknown fail closed, WiFi and Ethernet require `NOT_METERED`); blocked rows stay `pending` and re-pump on network change, with a `waitingForNetwork` event driving the "Waiting for WiFi" notice. Also wires the previously inert Smart Caching / Queue Pre-caching / WiFi Only settings toggles to `CacheConfig` | Downloads | UR-053 | Done (pending device verification) |
| DR-081 | `/downloads` split into a default **Downloaded** browse view and a secondary **Transfers** activity view, with a view switch and a Transfers badge shown only while transfers are active | UI | UR-055 | Done |
| DR-082 | Offline-scoped browse entry point in the repository client: browse downloaded content only (offline repository `get_items`/`get_libraries` — downloaded items plus their containers) independent of server reachability, without merging server catalog | Storage | UR-055 | Done |
| DR-083 | Downloaded browse reuses library grids, cards, and detail pages via the offline-scoped source; omits libraries/containers with no downloaded content; badges partially- vs fully-downloaded containers; play uses the local file; remove available at item/album/season/series level | UI | UR-055 | Done |
| DR-084 | Transfers view renders only in-flight rows (downloading/queued/paused/failed/waiting-for-WiFi) with Pause/Resume/Cancel/Retry; completed transfers leave the view and appear in Downloaded | UI | UR-055 | Done |
| DR-085 | Per-item on-disk size: stat downloaded files, aggregate to album/season/series subtotals and a device total, format in consistent rounded human units; surface size on cards and detail pages, the device total on the Downloaded surface, and a reclaim figure in the remove confirmation | Downloads | UR-056 | Done |
| DR-086 | Settings page persists each control on change via per-group writers (`playerSetAudioSettings` / `playerSetVideoSettings` / `updateCacheConfig`) rather than a batch Save action; slider controls persist on `change` (pointer release) not each `input` tick; no Save button, `saving`, or `saveMessage` state | Settings | UR-057 | Done |
| DR-087 | `MediaCard` gains an `onLongPress` prop with pointer-based long-press detection (~500 ms hold, cancelled on >10 px move so carousel scroll is unaffected, trailing click suppressed); home carousels wire tap→detail/focus routing and long-press→confirm→player; episode taps route to `/library/<seriesId>?episode=<id>`; the bare-episode detail page links to its parent series/season | UI | UR-058 | Done |
| DR-088 | Skip-to-next-episode marks the outgoing episode played (`markAsPlayed`) instead of reporting a stop position, and arms a one-shot suppression consumed by the player's stop handler so `VideoPlayer`'s post-navigation unmount stop report cannot overwrite the 100% progress with the partial position | UI | UR-059 | Done |
| DR-089 | Continue Watching suppresses resume entries superseded by Next Up: an in-progress episode whose series has a next-up entry strictly later in series order (season, then episode) is dropped from the Home and TV rows; movies, series without a next-up entry, and items with unknown/mixed episode ordering are always kept | UI | UR-059 | Done |
| DR-090 | Relevance ranking in Rust (`domain/search_rank.rs`): results sort by match position (prefix → word-start → mid-word substring → no name match) then by media kind (containers before their contents), stably so the backend's own relevance breaks ties. Applied in `repository_search` to both the instant cache result and the merged cache+server union, so the list does not reshuffle when server results land | Backend | UR-060 | Done |
| DR-091 | Search result groups split TV into separate Shows and Episodes groups and add a People group (default order: Shows → Episodes → Movies → Songs → Albums → Artists → People); a stored `tvShows` order from before the split expands in place to shows+episodes so an upgrading user keeps their arrangement | UI | UR-060 | Done |
| DR-092 | Video tap gestures resolve in `tapGestures.ts` (pure, unit-tested) rather than inline in `VideoPlayer.svelte`: `registerTap` classifies each tap and the component acts on it immediately — `togglePlayPause` for a first tap, or `seek` (+30 s right / −10 s left) plus a re-toggle for a second tap inside `DOUBLE_TAP_WINDOW_MS` (300 ms). A consumed pair resets the state, and a swipe forgets the tap. The deferral this originally used was removed in DR-098, which also covers suppressing the compatibility `click` the browser synthesizes after a touch tap. `resolveSeekTarget` converts the delta to the absolute position the facade requires, clamped per DR-095 and chained off a still-in-flight `pendingSeekTarget` so back-to-back skips accumulate instead of all resolving against a not-yet-updated position | UI | UR-061 | Done |
| DR-094 | Frontend boundary tripwire (`scripts/check-frontend-boundary.sh`) detects Jellyfin item-type array literals **anywhere** in `src/` rather than only inline at an `includeItemTypes:` query site, so a category→type mapping cannot evade the check by being assigned to a named const (the evasion that let the `scoped-search` leak pass CI); requires two adjacent type literals so single-type presentation and `item.type ===` inspection stay legal, and caps the allowlist to force taxonomy into Rust instead of accumulating exceptions | Tooling | - | Done |
| DR-098 | Video tap gestures act **immediately** — no deferral, no timer, and only first/second taps exist. A first tap toggles play/pause; a second tap inside `DOUBLE_TAP_WINDOW_MS` seeks *and* toggles again, so the two toggles cancel and a double tap preserves the play state (playing → jump and keep playing; paused → jump and stay paused). This replaces a design that deferred the first tap behind a 300 ms timer so a second tap could cancel it: the timer cleared its own handle *before* invoking the toggle, which reopened the `tapTimeout !== null` guard in `handleVideoClick` meant to suppress the compatibility `click` Android's WebView synthesizes after a touch — the late click then toggled a second time, producing a pause/unpause loop (long-press was unaffected, which is what identified the tap path). Click suppression no longer depends on the timer: `handleVideoClick` ignores `detail === 0` *and* any click within `TOUCH_CLICK_SUPPRESS_MS` of a touch tap. A swipe undoes the touchstart toggle exactly once (latched on `swipeGestureActive`) so brightness swipes never change play state. Click suppression is shared by **every** click target layered over the video via `isSynthesizedTouchClick`, not just the `<video>`: pausing renders a full-screen play-overlay button, so the synthesized click lands on *that* and an unguarded handler there resumed immediately — pausing appeared impossible while unpausing worked, because unpausing removes the overlay | UI | UR-061 | Done |
| DR-099 | The video seek bar is usable by touch. Two Android-only defects made dragging or tapping it move the thumb without moving playback. (a) *Gesture hijack*: the container-level gesture layer skips `touchstart` on a control (DR-098) but kept handling `touchmove`, so a seek-bar drag was measured against the **previous** gesture's start point — a huge bogus vertical delta that read as a brightness swipe, dimmed the screen to the 0.3 floor, and fired a spurious play/pause "correction" mid-drag. A gesture is now latched at `touchstart` (`playerGestureActive`) and `touchmove` ignores anything not latched, since re-checking the move target cannot recover a start point that was never recorded. (b) *Commit signal*: the seek was committed **only** from `change`, which Android's WebView does not reliably fire for a touch interaction on a range input — the thumb moved to the tapped position and no seek ever ran. `touchend`/`mouseup` now commit as well; `input` arms a one-shot latch so whichever release signal arrives first commits and the other is a no-op. `seekRelative` shares the same `commitSeek` entry point instead of fabricating a synthetic `change` event | UI | UR-005, UR-061 | Done |
| DR-097 | Transport authority (play/pause/toggle) lives in Rust for **webview-rendered** media, not just native. The controller tracks the state the HTML5 element reports (`html5_playing`, fed by `report_html5_state`, which now *stores* rather than only re-emitting); `play`/`pause`/`toggle_playback` consult it and drive the element by emitting a `ControlCommand` that `playerEvents.handleControlCommand` executes against the active adapter. A `stopped`/`idle` report clears it so the native backend (MPV/ExoPlayer) regains authority for music. The frontend facade no longer short-circuits transport into the adapter: `adapter.toggle()` previously decided play-vs-pause by reading `el.paused` off the DOM, a value that flips transiently while an element buffers or settles a seek — so two intents ~150 ms apart read *different* values, performed *opposing* actions, and self-sustained a play/pause loop needing no further input (observed on Android with a fully-buffered `readyState=4 networkState=1` element). Same "backend decides, adapter executes the primitive" split as `player_seek_video` | Player | UR-005 | Done |
| DR-096 | `Html5PlayerAdapter.play()` is resilient to stall recovery: an in-flight attempt is memoised so concurrent callers (UI plus hls.js gap-controller recovery) share one `element.play()` instead of stacking calls, and an `AbortError` ("play() request was interrupted by a call to pause()") is logged at debug rather than pushed to `host.onError`. The browser raises it whenever a pending play promise is superseded by a pause/seek/source change, which hls.js does routinely while nudging past a stall — reporting it surfaced a player error roughly once per second for the whole stall and left the UI stuck showing paused | Player | UR-005 | Done |
| DR-095 | Seek targets clamp strictly *inside* the media (`clampSeekTarget`, `END_SEEK_MARGIN_SECONDS` = 6 s ≈ one HLS segment) instead of to the exact `duration`. Landing on the duration makes hls.js request the segment whose start time lies past the end of the media (e.g. a 6330.324 s item → segment 1055 starting at 6336.33 s), which Jellyfin never produces; the fetch times out and hls.js' gap-controller stalls at the last buffered position, presenting as "unpausing or skipping bounces straight back to paused". Applied on both seek paths — the relative-skip `resolveSeekTarget` and the seek-bar drag, whose range input `max` is the duration itself — and floored at 0 so media shorter than the margin still seeks to the start | UI | UR-061 | Done |
| DR-100 | Leaving a video and re-entering it renders the **video** player, never the audio one. Both halves of the `/player/[id]` decision are pure and unit-tested in `playerSurface.ts`. (a) `shouldReuseActivePlayback` excludes video: the "already playing, just show the UI" shortcut (added for expanding the audio mini player) returns *before* a stream URL is fetched, which is fine for audio — the backend owns the stream and the route only mirrors it — but leaves `<VideoPlayer>` with nothing to render. Closing a webview-rendered video deliberately emits no `stopped` state (that would break the autoplay handoff, see DR-047), so the Rust controller still reports that movie/episode as its loaded media and re-entering the same item hit the shortcut. (b) `resolvePlayerSurface` maps video-without-a-stream-URL to `pending` (spinner) instead of falling through to `<AudioPlayer>`, so no future path can put video content in the audio surface. Video now always takes the full load path, which fetches the stream URL and applies the stored resume position | UI | UR-005 | Done |
| DR-101 | "Where is this viewer in this series" is resolved in **Rust**, not the frontend. `repository_get_series_episodes` performs the season fan-out (`get_items(series_id)` → seasons → `get_items(season_id)`, plus the flat-series fallback for shows whose children are episodes rather than season folders) and returns them in series order — season index ascending, episode index ascending, specials (season 0) after every numbered season. `repository_get_series_current_episode` layers the pure policy `pick_current_episode` over that list: an **in-progress** episode wins (earliest in series order on a tie — it is literally where playback stopped, and Next Up would skip past it), then the server's **Next Up** for that series, then the **first unwatched** episode, then the first. The third rung is the offline path, not dead code: `OfflineRepository::get_next_up_episodes` returns an empty vec, so without it the feature would be online-only. A failing Next Up or resume lookup degrades to empty rather than failing the call. `repository_get_next_up_episodes` had accepted a `series_id` since it was written and **no caller had ever passed one** | Repository | UR-062 | Done |
| DR-102 | The series detail page anchors on that answer. It calls `repositoryGetSeriesEpisodes` once instead of fanning out over seasons in TypeScript (the fan-out *and* its flat-series fallback were domain knowledge in the presentation layer), groups the returned episodes under season headers by `parentIndexNumber`, and passes the resolved current episode to `SeasonSection` → `EpisodeRow`, which renders a highlight ring and scrolls itself into view. The hero button navigates to `/library/<seriesId>?episode=<currentId>` — the Episode Focus View, where an explicit Play/Resume commits — per ux-flows §5B.5: Play on a *container* is navigation, Play on a *leaf* commits. It previously resolved `$libraryItems[0]`, the first **season** by `SortName`, and navigated to `/player/<seasonId>`, which the player route bounced back to `/library/<seasonId>` — so Play on a series played nothing and landed on the season-1 page | UI | UR-062 | Done |
| DR-103 | A season is not a destination. `/library/<seasonId>` redirects to `/library/<seriesId>#season-<indexNumber>`, the anchor `SeasonSection` renders, so a season link scrolls the series' continuous episode list rather than opening a page. Every inbound link follows: the episode breadcrumb, `handleItemClick case "season"`, the TV landing page's `case "Season"`, and `DownloadedBrowse`. A season carrying no `seriesId` (deep link into a stale cache) still renders the generic view so the user is never stranded. This removes a surface that had no route of its own — it fell through the detail page's `kind` chain to the generic "Contents" poster grid, contradicting ux-flows §5A.2 (episodes must be a row list), and clicking an episode there opened a bare Episode page, which §5B.1 forbids | UI | UR-062 | Done |
| DR-104 | The "More Episodes" strip spans the **whole series** in series order, per ux-flows §5B.2's cross-season continuity rule: at the end of a season the window runs on into the next season's first episodes instead of dead-ending. `adjacentEpisodes` previously filtered the pool to `parentIndexNumber === current.parentIndexNumber` and sorted by `indexNumber` alone, so the window could never leave the current season — and, when episodes of several seasons did reach it, sorting by episode number alone interleaved them. Cards crossing a season boundary are labelled `SxEy` rather than a bare episode number so the jump is legible | UI | UR-062 | Done |
| DR-105 | Video library routes collapse to one per library. `/library/tv` and `/library/movies` render browse / all-titles / genres as in-page tabs driven by `?view=`, omitted for the default `browse` (the convention `searchRouteUrl` already uses for the `all` scope); `resolveLibraryView` is pure and unit-tested. The four legacy routes become redirect-only `+page.ts` loads rather than deletions, because `GenreTags` links to them and users have them in history; `resolveSearchScope` keeps its `/library/shows` branch for the same reason. The "Browse" tile grid at the bottom of both landing pages is removed — it was a second navigation affordance to the same destinations the carousels' "Show all" links already reach | UI | UR-063 | Done |
| DR-106 | Erasing watch history goes through the repository, not the local cache: `clear_watch_history(item_id)` maps to Jellyfin's `DELETE /Users/{userId}/PlayedItems/{itemId}`, which clears the played flag *and* zeroes the resume position, and which the server applies recursively to a folder — so one call handles a whole series or season. `OfflineRepository` returns `RepoError::Offline` rather than clearing locally, because history diverged only on the device would be silently undone by the next sync; the button disables itself while the server is unreachable. `ClearHistoryButton` is shared by the series hero and each `SeasonSection` header, confirms before acting (there is no undo), and reloads the page on success so the recomputed current episode — the premiere, for a fully cleared series — is what the viewer sees | Repository | UR-064 | Done |
| DR-107 | Seasons on the series page are collapsible, and **only the current season is expanded** on load — the one holding the episode DR-101 resolved. A show with ten seasons otherwise renders every episode of every season at once, burying the one episode the viewer came for under hundreds of rows. Expansion state is per season and pure (`initialExpandedSeasons` in `seriesNavigation.ts`): the current season, or the first season when there is no current episode, so a never-watched show still opens on season 1 rather than fully collapsed. A `?episode=` deep link expands that episode's season too. Toggling is local and not persisted — it is a reading position, not a preference | UI | UR-062 | Done |
| DR-108 | The instant (cache) leg of `repository_search` searches the **synced catalog**, not just downloads. `OfflineRepository::search` replaces its `downloaded_items` CTE with the `available_items` CTE `get_items` already uses — the same downloads branches plus a `synced_at IS NOT NULL` branch gated on the same `include_catalog_browse()` flag — so search and browse cannot diverge on what is visible. Online (flag true) search reads the whole index and answers before any HTTP request completes; offline with "Show all server media" off (flag false) it stays downloads-only, unchanged. Requires no frontend change, since the flag is already set correctly for all three states. The `include_item_types` filter is switched from string interpolation to bound parameters, as `SearchOptions` is settable from the frontend and not only from `SearchScope` | Backend | UR-065 | Implemented |
| DR-109 | Index freshness is a Rust-owned policy, not a frontend startup call. A tokio task ticks every 30 min and runs a full pass when a repository is active, the server is reachable, and `last_catalog_sync` (already persisted to `app_settings`, previously read only for a UI hint) is older than `CATALOG_INDEX_TTL` (6 h); the `ConnectivityMonitor` reconnect signal re-evaluates the same condition immediately. An `AtomicBool` prevents concurrent passes, replacing `offlineCatalog.ts`'s `syncInProgress` — the frontend trigger is removed rather than left alongside, since two triggers with one guard each is how double-crawls happen. `RepositoryManager` gains an active-handle slot so the task has something to run against. Progress is emitted as the kebab-case `catalog-index-event` | Backend | UR-065 | Implemented |
| DR-110 | Index hygiene. `save_to_cache` switches from `INSERT OR REPLACE INTO items` to `ON CONFLICT(id) DO UPDATE`: REPLACE fires no `AFTER DELETE` trigger unless `recursive_triggers` is on (it is not — only `foreign_keys` and `journal_mode` are set), so `items_ad` never ran, and because `items.id` is a `TEXT PRIMARY KEY` each replacement also took a fresh rowid and appended a second `items_fts` entry — a duplicate index per sync, invisible in results but permanently degrading `MATCH`. The upsert preserves the rowid `items_fts` keys on and fires `items_au`; migration `021_rebuild_items_fts` clears orphans on existing installs. Separately, a post-crawl sweep deletes synced-but-not-downloaded rows a successful library crawl did not return, so media removed from the server stops being searchable; it skips items with completed downloads and skips any library whose crawl errored, because `items.parent_id` is `ON DELETE CASCADE` and a partial crawl would cascade away a whole series | Storage | UR-065 | Implemented |
| DR-111 | The index covers what the result groups render: `CATALOG_ITEM_TYPES` gains `MusicArtist` and `Playlist`, and migration `022_people_fts` adds a `people_fts` virtual table over the existing `people` table (which had no FTS, and is populated incidentally by item-detail fetches) with the same trigger pattern as `items_fts`. `OfflineRepository::search` UNIONs `people_fts` matches in as `Person` items when the resolved scope admits them — i.e. `SearchScope::All`, which expands to no filter (DR-063). Without this, the Artists and People groups UR-060 mandates can only ever be filled by the server leg | Storage | UR-065, UR-060 | Implemented |
| DR-112 | Safe-area insets come from **native**, not from `env()` alone. `env(safe-area-inset-*)` is 0px without `viewport-fit=cover` (missing from `app.html`, so every safe-area rule in the app was already a no-op), and even with it Android WebView maps only the *display cutout* — never the status bar or navigation bar. Since `enableEdgeToEdge()` plus `targetSdk 36` make edge-to-edge unconditional, the WebView always spans the system bars, so CSS could not learn about them by any route. `WindowInsetsBridge` reads the real insets and publishes `jt-inset` custom properties; `app.css` folds them with `env()` via `max()` into `--safe-*`, which is the only thing components may pad from. Ownership is exactly one element per edge: the app shell takes top/left/right, and BottomUi takes bottom wherever it renders (`shellReservesBottomInset` hands it back to the shell on routes with no bottom UI) so the padding sits inside BottomUi's surface box and the colour extends behind the gesture bar. The full-screen players inset their control layers only, leaving video and artwork edge-to-edge. The theme's `fitsSystemWindows=true` — which claimed the opposite and was overridden at runtime and ignored at this target SDK — is removed | UI | UR-066 | Done |
| DR-113 | `MediaItem.user_data` is populated from the server instead of being hardcoded `None`. `JellyfinItem` gains a `UserData` field (`#[serde(alias = "UserData")]` → the existing `UserData` type) and `to_media_item` maps it, so every list and detail response carries favourite/played/resume state. `UserData` is named explicitly in the `Fields=` list rather than relying on Jellyfin's default. Without this no card or detail page can render a favourite it did not itself set, and the mini player's per-track `storageGetPlaybackProgress` fetch is the only way to colour one heart | Repository | UR-069 | Done |
| DR-114 | Server favourite state is mirrored into the local `user_data` table by `OfflineRepository::save_to_cache` — the single choke point every cached server result passes through — so offline browsing and the offline Favourites page see the same favourites as the server. The upsert carries `pending_sync = 0` and is guarded by `WHERE user_data.pending_sync = 0`, which is the conflict rule: a toggle made offline is never overwritten by a stale server value before it has been pushed | Storage | UR-069 | Done |
| DR-115 | Cross-library favourites query: a `get_favorites(scope, options)` repository method plus the `repository_get_favorites` command. Online issues `Filters=IsFavorite&Recursive=true` with `IncludeItemTypes` expanded from `SearchScope::item_types()` in Rust (the frontend sends the opaque scope, never a type list — DR-063); offline reads `items ⨝ user_data (is_favorite = 1)` under the same `include_catalog_browse()` gate as browsing; hybrid races cache against server like `get_items` — saving server results through to the cache on a miss, so the favourites page does not re-query the server every visit and the DR-114 mirror is filled on a fresh install — and applies the DR-080 rule that an empty offline result is authoritative when the gate is off. The command falls back to this read when nothing is cached, rather than painting an empty state it will correct a round trip later. A separate method rather than `get_items` because favourites span libraries and `get_items` is `ParentId`-shaped | Repository | UR-067 | Done |
| DR-116 | `GetItemsOptions.favorites_only` filters an existing library listing in place — online by appending `Filters=IsFavorite`, offline by joining `user_data` into the existing `available_items` CTE so the downloads-only gate still applies. This is what backs the per-library favourites toggle, and composes with the genre and item-type filters already there | Repository | UR-067 | Done |
| DR-117 | The Favourites page (`/library/favorites`) renders favourites across libraries with All / Movies / Shows / Music scope tabs, reusing `LibraryViewTabs` + `LibraryGrid` + `MediaCard` so card shape still follows the media (§5A.1) and a mixed All tab reads as posters, squares and thumbnails side by side. Each tab sends a `SearchScope` value and nothing else. Reached from the library overview and from "See all" on the home rows | UI | UR-067 | Done |
| DR-118 | Home carries favourite rows for movies, shows and music, loaded via `repository_get_favorites` per scope and rendered below Recently Added. A row with no items does not render at all, so a fresh install shows no empty favourite rows | UI | UR-067 | Done |
| DR-119 | `FavoriteButton` is mounted wherever a whole item is shown — movie/series/episode detail heroes, album/artist/playlist headers, and as a `MediaCard` artwork overlay — and a `favorites` store holds in-session optimistic state so un-hearting on one surface updates every other without a refetch. Resolution order is `store override ?? item.userData?.isFavorite ?? false`. On a card the heart is its own button and stops propagation, so hearting never also opens, plays, or triggers the §5B.5 long-press; it is suppressed on server-only (greyed) cards | UI | UR-068 | Done |
| DR-120 | Favourite toggles made while offline reach the server. A Rust drain, triggered by the `ConnectivityMonitor` offline→online transition, pushes every `user_data` row with `pending_sync = 1` and clears the flag on success, leaving failures pending for the next transition. It lives in Rust rather than the frontend because a frontend drain dies with the component that started it. Both the drain and the hybrid background refresh emit the kebab-case `favorites-changed` event (`{ itemIds }`) so open views update — without it a favourite marked on another client appears only on the *second* visit to a page, since the cache-first read returns local rows and the server refresh is invisible to the frontend. Supersedes the unused `syncService.queueFavorite`, which is deleted rather than left as a second queue | Backend | UR-069 | Done |
| DR-121 | Player quality selector: Rust reports the bitrates available for the current media source and owns the quality→transcode-parameter mapping (the one `get_video_download_url` already holds — playback calls into it rather than restating it, or the two tables drift). Changing quality re-negotiates the stream URL and resumes at the current position with audio/subtitle selection preserved. On Linux, video re-negotiates *within* HLS: returning `stream.mp4` is the documented cause of transcoded playback never starting. The frontend renders the list and remembers the choice; it does not decide what the choice resolves to | UI | UR-070 | Proposed |
| DR-122 | The playback path is ephemeral. Streamed bytes are never persisted unless DR-124 rules them keepable, and any in-flight capture is abandoned — partial file deleted, never promoted — the moment the viewer changes quality, because a capture spanning a rendition change is a splice of two encodings rather than a playable file | Playback | UR-070 | Proposed |
| DR-123 | The download path is independent of playback: a whole-file fetch through the existing download manager at one canonical quality (default `original`, the direct static copy) over the Range-capable `/Videos/{id}/stream.mp4`, unaffected by bitrate changes and completing into an ordinary `downloads` row so offline browsing and `refresh_queue_local_sources` pick it up unchanged. Prerequisite: downloaded video is currently never played locally — `repository_get_video_stream_url` goes straight to the online repo and the player route calls it with no local check, so a completed video download is still streamed. Without that fix nothing in this spec is observable for video | Repository | UR-071 | In Progress |
| DR-124 | Streamed bytes are kept only where they *are* the download artifact — a direct-play session. Android uses ExoPlayer `SimpleCache`/`CacheDataSource` keyed by item **and** media-source id so renditions cannot collide, sharing the existing smart-cache storage budget rather than opening a second one over the same disk; Linux audio uses mpv `stream-record`, abandoned on seek because it is documented as intended for linear streams and seeking breaks the recording. Transcoded Linux video is **not** captured: HLS segments are not a file, and assembling one needs ffmpeg, which is not a dependency and which CI may not install at job time — DR-123 covers that case instead | Playback | UR-071 | Proposed |
| DR-125 | A capture is promoted to a completed `downloads` row only when it covers the whole resource; partials stay evictable cache. A new `downloads.source_rendition` column records the negotiated quality/container/codec (`NULL` for the existing paths, which are always `original`) so a captured transcode and a real download are distinguishable rows and an "upgrade to original" remains possible. A quality change never touches a file that already exists — not a permanent download, and not a completed temporary one, both of which stay valid copies of the rendition they hold. It invalidates only an **in-flight** capture or background download of cached media, which is abandoned and restarted at the newly chosen quality, because a capture spanning a rendition change is a splice of two encodings rather than a playable file | Storage | UR-071 | Proposed |
| DR-126 | Cache eviction only reclaims the *temporary* tier. `evict_lru_async` selected every completed download ordered by `completed_at ASC` with no `download_source` filter, so hitting the 10 GB storage limit deleted the **oldest** download — typically a film saved deliberately for offline — to make room for a newly precached track. It now evicts only `COALESCE(download_source, 'user') = 'auto'` rows; `COALESCE` rather than a bare equality because rows predating migration 012 can be NULL and unknown provenance must be treated as the user's, never as disposable. Freeing less than requested is the correct outcome when only user downloads remain — the caller reports "unable to free enough space" instead of silently deleting them | Storage | UR-071 | Done |
| DR-127 | A cache entry *is* a download with a shorter life: same `downloads` row and same file handling, distinguished by `download_source = 'auto'` plus an expiry, so there is one storage model rather than a cache and a download library that can disagree. Temporary rows are reclaimed on whichever comes first — the life limit elapsing, or eviction under space pressure (DR-126). Permanent (`'user'`) rows have no expiry. A temporary row can be promoted to permanent by the user choosing to keep it, which only clears the expiry and flips the source; the bytes never move | Storage | UR-071 | Done |
| DR-128 | Audio-only playback of *downloaded* media reads the local file rather than fetching an audio-only stream. No transcode is involved or wanted: the Linux backend already runs MPV with `video: no`, so handing it the downloaded video file decodes the audio track and ignores the video, and ExoPlayer disables its video renderer equivalently. Transcoding to a separate audio artifact would cost CPU and battery, need an encoder the project does not ship, and produce a second file to keep in step — for no gain over simply not decoding the video | Playback | UR-071 | Done |
| DR-129 | A stream that stops delivering is recovered, not treated as terminal. Two failure shapes, because the streams differ. (a) *Phantom end* — the background audio-only handoff uses a progressive mp3 transcode over plain HTTP, chunked and therefore length-less, so a dropped connection reaches the player as end-of-input and ExoPlayer reports `STATE_ENDED` indistinguishably from the real end. The item's runtime is the only thing that can tell them apart: an end reported more than a tolerance short of it (comparing the *absolute* position — handoff base plus the player's relative position) is a truncation. Left unhandled, playback parked in `STATE_ENDED` and the next play intent from the lockscreen, notification or a Bluetooth reconnect seeks an ended player to position 0 — the user-visible "the episode randomly restarted". (b) *Recoverable error* — music (`/Audio/{id}/stream?Static=true`) and video (`/Videos/{id}/master.m3u8`) declare their length, so the player detects the truncation itself and raises an error; the frontend's handler stopped playback outright, turning a hiccup into silence. Both resume the current item **in place** (never via `play_item`, which would replace the queue with a single item and lose the album), the error path after a per-attempt backoff. Seekable streams are re-prepared at the URL they already have and seeked; the length-less transcode, which cannot be seeked, has `StartTimeTicks` rewritten into its existing URL so the user's audio-track selection survives and recovery needs no network round-trip. Only `Remote` sources qualify — a local file cannot fail from the network. A shared budget of consecutive attempts at the same position, refilled whenever playback progresses, stops an unreachable server from looping | Playback | UR-040, UR-004 | Done |
| DR-130 | A backend's position and duration must survive the end of the file they describe. MPV exposes `time-pos`/`duration` as properties of the *loaded* file, so at EOF it unloads and both stop resolving — the accessors reported `0.0`/unknown at exactly the moment end-of-file handling asks where playback reached, and any position-versus-runtime check would have read every natural end as a truncation. The poll thread records the last reading and the accessors fall back to it. Linux resilience is layered on the same principle that the stream, not the player, is what failed: MPV is configured with ffmpeg reconnection (`stream-lavf-o`, `network-timeout`) so ordinary blips never surface, and `EndFile(ERROR)` — previously a bare log, which left playback halted while the UI still showed "playing" — is emitted as a *recoverable* error. Because MpvBackend is constructed before `PlayerController` exists, it cannot decide in-process like the Android JNI callback: the frontend echoes the error into `player_recover_stream`, which keeps the decision in Rust (the same shape as `PlaybackEnded` → `player_on_playback_ended`). Android reports errors it has already declined as *unrecoverable*, so the echo never asks twice | Playback | UR-004, UR-040 | Done |
| DR-131 | The offline mutation queue is drained. `sync_queue` had producers and no consumer: `PlaybackReporter::queue_for_sync` writes a row for every start/stop/mark-played that cannot reach the server, `sync_mark_processing`/`_completed`/`_failed` were registered commands with no callers, and no Rust task processed the table — so queued watch positions never reached Jellyfin and the offline banner's count only ever grew. A drain hangs off the same `connectivity:reconnected` transition as DR-120 (in Rust, because a drain started by a component dies with it) and replays rows oldest-first, so a stale start cannot move the server's resume position backwards after a later stop. `update_progress` replays as *stopped at N* rather than as progress — replaying a mid-playback report hours later would claim the item is still playing — and payloads are read in both dialects that exist in users' databases (`position_ticks` from Rust, camelCase `positionMs` from the frontend helper). A failed row stays queued for the next reconnect; after `MAX_SYNC_ATTEMPTS` it is `abandoned` and stops counting, because a row nothing can ever push is what turns the queue into a counter that only grows. An *unreachable* server is not counted as an attempt at all — the row goes back to `pending` untouched — so opening the app offline a few times cannot abandon good rows; only a server that answers and refuses spends the budget. The drain also runs once at startup, because a queue built in a previous session would otherwise sit untouched for a whole run whenever the server was reachable the entire time and no offline→online transition ever fired. Requires `MediaRepository::mark_played` (JA-035) — the previous stand-in reported a stop at `i64::MAX` | Backend | UR-025, UR-002 | Done |
| DR-132 | The pending-sync count is answerable. The offline banner's badge read "N pending sync(s)" and led nowhere, so it was taken for pending *transfers* and looked for on the Downloads page — which lists the `downloads` table and structurally cannot show `sync_queue` rows. The badge becomes a button opening the queue it counts: each row's operation, the item's title (resolved by a `LEFT JOIN items` in `sync_get_pending`, not a per-row frontend fetch), when it was queued, and the error of anything failing, plus a "Sync now" that runs the DR-131 drain on demand. The same list is a Settings section, because a row that keeps failing is still queued when the server is reachable and no banner is on screen. The drain emits `sync-queue-changed` so the badge updates on reconnect instead of lagging by up to one 10s poll | UI | UR-025 | Done |
| DR-133 | A downloaded file has exactly one on-disk path, and the row that names it is authoritative. `downloads.file_path` starts relative to the storage root, but the worker rewrites it to the absolute path it actually wrote when the transfer completes — so a *completed* row is already rooted. The video player's offline branch rooted it a second time, handing the asset protocol `/data/user/0/app//data/user/0/app/videos/x.mp4`; the webview reported `MEDIA_ERR_SRC_NOT_SUPPORTED` with `NETWORK_NO_SOURCE`, so every downloaded video failed to play while audio — which resolves the same column through Rust's `resolve_local_media_path`, without re-rooting — played fine. The join is absolute-aware (POSIX, Windows drive letters and UNC) so rows written before completion still resolve | Playback | UR-071 | Done |
| DR-134 | The webview can actually fetch the local files it is handed. `convertFileSrc` rewrites a path to `http://asset.localhost/…` unconditionally, but Tauri only answers that origin when the `protocol-asset` cargo feature is compiled in *and* `app.security.assetProtocol.enable` is set — neither was, so every such URL reached a protocol with no handler and the webview reported `NETWORK_NO_SOURCE`. This silently defeated both offline video (`<video src>`) and the cached-thumbnail path in `imageCache`, which fails soft to the server copy and so hid the breakage whenever the server was reachable. The scope is `$APPDATA/**` — the storage root under which the database, `downloads/` and the thumbnail cache all live — rather than an unrestricted grant, so the webview can read the app's own media and nothing else | Security | UR-071 | Done |
| DR-140 | An audio track is pinned only when the user picked one. Jellyfin's `MediaStream.Index` is global across every stream in a media source, so index 0 is the *video* stream on virtually all files — yet `AudioStreamIndex=0` was sent as "the first audio track" on the HLS transcode URL, the background audio-only handoff URL, the direct-play fallback URL, and the `PlaybackInfo` negotiation body. A server that honours the request literally then transcodes the video stream into the audio slot and the result plays as a picture with no sound; only servers that silently correct the index hid the bug, which is why it presented as "some videos have no audio". The parameter is now omitted whenever no track has been chosen, so the server resolves the source's `DefaultAudioStreamIndex`; an explicit selection from `player_switch_audio_track` is still carried through unchanged. On the `static=true` direct-play URL it is dropped outright — the original file is served untouched, so the parameter could only mislead | Playback | UR-004, UR-040 | Done |
| DR-147 | One search input per screen, and the URL is the search's single source of truth. The header bar rendered only under `/library/**` and merely *navigated* to `/search` (DR-063), so a desktop search handed the user to a screen whose input was a different element — the header box cleared itself and vanished, and the page's own box took over mid-word. That page then re-derived its input from `?q=` against `library.searchQuery` on every store write, so the next keystroke re-ran the effect and snapped the text back to the query the header had sent (and a scope chip back to the URL's scope); entering from the bottom-nav Search tab skipped it only because the effect early-returned on an empty query. The bar now renders on `/search` too (`showHeaderSearch`) and is the sole md+ input — the page's own input is `md:hidden` — and on that route it republishes the query into the URL with `replaceState`, so a whole session of typing costs one history entry. The page *consumes* that URL once per distinct value (`seedFromSearchUrl` against a non-reactive `applied` marker) instead of continuously reconciling it, and the scope chips publish through the same URL so the bar and the chips cannot disagree. Landing on `/search` with a seeded query focuses the bar and puts the caret at the end, because the box the user was typing in belonged to the unmounted route | UI | UR-049, UR-054 | Done |
| DR-142 | An episode has exactly **one** surface, and it is complete. Two divergent renderings existed: `EpisodeFocusView` (reached from Continue Watching, the series episode list, the TV landing page and Downloads — i.e. every real entry point) offered only Play and Favourite, while the bare `/library/<episodeId>` page nobody routed to carried the download button, the series/season breadcrumbs and the cast section. Opening an episode the normal way therefore silently lost the ability to download it. The Focus View is now the single surface and carries the full §5B.2 composition — hero action row `Play / Download / Favourite`, series name and `SxEy` badge as links back to the series and to that season's anchor, then genres → cast → similar shows *below* the episode strip, never above it (DR-062). `/library/<episodeId>` redirects into it (`episodeRedirectTarget`, the same rule seasons follow under DR-103), and an episode with no `seriesId` renders the same component series-less rather than falling back to a second, lesser page. The focused episode is fetched in full rather than reused from the season fan-out, because that is a *list* query and carries neither cast nor genres — the sections would have rendered empty. The strip hides itself when the episode has no siblings, a card that only shows the episode you are already on being noise | UI | UR-048, UR-058 | Done |
| DR-141 | The device profile states how many channels the audio route can actually voice. `MediaCodecList` answers "can this device *decode* 5.1", which is not the question that decides whether the user hears anything — a phone decodes an AC-3 5.1 track happily and still has two channels to play it out of. With no `MaxAudioChannels` in the profile, Jellyfin was free to direct-play the multichannel track, and the result is device dependent: a failed `AudioSink` configuration (silence) or dialogue folded into surround channels that go nowhere. media3's `AudioCapabilities.maxChannelCount` for the current route is reported over JNI alongside the codec lists, and bounds both the direct-play profile and the transcoding profiles, so the server downmixes rather than shipping channels the sink cannot take. Codecs are never removed from the profile — a device with genuine surround output keeps direct-playing it. A missing or zero reading means "route not yet established", not "no audio", and falls back to stereo, the one capability every sink has | Playback | UR-004 | Done |
| DR-145 | Video playback starts only once the app actually holds audio focus. Video manages focus by hand (`handleAudioFocus=false`, because ExoPlayer's automatic handling is reserved for the audio path), and the request's three outcomes were all treated as success: `AUDIOFOCUS_REQUEST_DELAYED` — which `setAcceptsDelayedFocusGain(true)` explicitly invites, and which means the system is *withholding our audio* until it calls back — and an outright `REQUEST_FAILED` were logged and then followed by `playWhenReady = true`. The picture rolled with no sound, indistinguishable to the user from a broken stream. Playback is now held when focus is not granted and started from the `AUDIOFOCUS_GAIN` callback; an explicit `play()` re-requests focus rather than resuming into a stream the system is still muting, guarded by a held-focus flag so repeated plays do not leak focus requests. A `LOSS` clears the pending flag, so an unrelated later `GAIN` cannot start playback the user never asked for | Playback | UR-004 | Done |
| DR-146 | The no-audio-track fallback picks a track the renderer can actually play. When ExoPlayer selected no audio track, the recovery forced group 0 / track 0 unconditionally — but the most likely reason nothing was selected is that this very track cannot be decoded on this device, so the override reinstated the silence it was meant to fix. It now scans the groups for the first `isTrackSupported` track and overrides to that, and clears `setTrackTypeDisabled(TRACK_TYPE_AUDIO)` because audio may equally have been off at the type level, which an override alone does not undo. When no group holds a supported track the condition is logged as an error — the server was expected to transcode — rather than leaving a silent video with no explanation in the log | Playback | UR-004 | Done |
| DR-148 | The video direct-play profile advertises only what the **webview** can decode. The audio codec list comes from `MediaCodecList`, which describes ExoPlayer — but video does not play through ExoPlayer on either platform: Android force-renders every video in the webview `<video>` element (the interim override in `VideoPlayer.svelte`, because the native SurfaceView sits behind an opaque webview) and Linux always has. Chromium and WebKit decode a far narrower set than the platform does, and the gap is widest on devices whose vendor licenses Dolby: a phone shipping `/vendor/etc/media_codecs_dolby_audio.xml` reports `ac3,eac3`, so Jellyfin direct-played an E-AC-3 track with `static=true` and the webview built a video decoder and no audio decoder at all — full picture, no sound. The defect is triggered by *capability*, not the lack of it, which is why it reproduced on one Motorola while a Fairphone and an Honor tablet played the same file on the same build: a device without the Dolby decoder never claims the codec, so the server transcodes to AAC and it plays. `video_audio_codecs` narrows the platform list to the webview-decodable set (`aac,mp3,opus,vorbis,flac`) for the video direct-play profile *only* — the audio-only profile keeps the full list, since that playback really is the native player's and narrowing it would transcode music that plays perfectly well. A list with nothing decodable still claims `aac` rather than going out empty, because a profile that claims nothing invites the server to give up instead of transcoding. The video codec list is deliberately untouched: HEVC direct-plays through the webview correctly, so the constraint is specific to audio | Playback | UR-004 | Done |
| DR-149 | The client decides whether its own renderer can decode the audio, rather than trusting the server's negotiation. Advertising a webview-shaped profile (DR-148) turned out to be necessary but not sufficient: Jellyfin 10.11.5 enforces a `DirectPlayProfile`'s `Container` and `VideoCodec` — excluding either returns `SupportsDirectPlay: false` with `TranscodeReasons=ContainerNotSupported` / `VideoCodecNotSupported` — but **ignores its `AudioCodec`**, offering an E-AC-3 track for direct play against a profile listing only `aac,flac,mp3,opus,vorbis`. Neither a `VideoAudio` `CodecProfile` forbidding the codec nor a `MaxAudioChannels: 2` against a 6-channel track changes the answer, so no profile the client can send fixes it and the picture plays silent. The negotiated source's audio is therefore checked locally against what the webview decodes, and an undecodable track forces the existing h264/aac HLS transcode URL regardless of the server saying direct play is fine — `direct_play` and `needs_transcoding` are corrected to match, so the frontend and the reporting path agree with the URL actually used. The track judged is the one the server would serve: the default, or the first when nothing is marked default, since a supported track further down the list is not the one that plays. A source with no audio streams, or a stream whose codec the server did not name, is left alone — forcing a transcode on a guess spends server CPU on files that already play | Playback | UR-004 | Done |
| DR-150 | Android video renders on the native ExoPlayer surface behind a transparent WebView, behind the `experimentalNativeVideo` opt-in. Rust already reported `use_html5_element: false` on Android, but two frontend overrides discarded it — `createAdapter()` hardcoded `"html5"`, and `VideoPlayer.svelte` forced `useHtml5Element = true` and stopped the native backend `player_play_item` had just started. The flag is a **suppressor, never a promoter**: off forces HTML5 even where Rust says native, so an in-progress spike cannot ship as the default, but it can never select native where Rust reported HTML5 (Linux cannot composite behind WebKitGTK, so promoting there is a black screen). Compositing requires clearing two independent opaque layers, and clearing only one leaves audio over a black picture — the WebView widget background and window drawable from Kotlin (`AndroidVideoSurface.setTransparent`), and the page's `html`/`body` and app-shell background from CSS (`data-native-video`). Transparency is declared in `tauri.android.conf.json` rather than the base config, because a transparent window on Linux has nothing behind it, and is toggled per playback session rather than set once, because a permanently transparent window shows the launcher through the rest of the app | Playback | UR-003, UR-004 | Done (behind `experimentalNativeVideo`, default off) |
| DR-151 | The player's video SurfaceView actually reaches the view hierarchy. `JellyTauPlayer.setActivity()` had zero callers, so `currentActivity` was always null and `autoAttachSurface()` returned at "Cannot attach surface - no Activity reference". The surface was created and handed to ExoPlayer but never added to the content view, so native video decoded to a surface that was never on screen — independent of any webview transparency. `MainActivity.onCreate` now supplies the reference, which also revives PiP on the video path: `canEnterPip()` gates on `isVideoSurfaceAttached()`, which had been permanently false | Playback | UR-003, UR-041 | Done |
| DR-152 | Platform playback facilities are reported by Rust, not sniffed from the user agent. `webviewAudio.ts` re-derived "does this platform have a native audio backend" by matching `navigator.userAgent` against `android`/`linux` — a second copy of the `cfg!` gate the backends are compiled under, free to drift from it. `player_get_capabilities` now returns `usesWebviewAudio` and `supportsNativeVideo` from the same cfg gates, and the frontend consumes them; the settings toggle for native video is hidden entirely where the platform cannot support it | Player | UR-003, UR-005 | Done |
| DR-153 | The git tag is the single source of truth for a release version. The version lived in four files (`package.json`, `tauri.conf.json`, `Cargo.toml`, `Cargo.lock`) that had to be hand-edited in lockstep, and CI's release job rewrote exactly one of them — so a tagged build produced an installer named for the tag wrapped around package metadata naming the previous release, while the Linux job had no version step at all and shipped whatever was committed. `scripts/set-version.sh` writes all four from one argument and is the only thing that does; every release job calls it with the tag. The Android `versionCode` is derived in the same place as `1000 + major*10000 + minor*100 + patch`, which is monotonic in semver order and clears the 1000 floor already installed in the field — a lower code than the installed one makes Android refuse the update. A prerelease suffix is stripped before that arithmetic, which would otherwise abort the script, and a non-tag ref (CI passes `${GITHUB_REF#refs/tags/}` unconditionally) falls back to `git describe` rather than failing a branch build | Build | - | Done |
| DR-154 | A watch position that cannot reach the server is queued, not dropped. `sync_queue` and its drain (DR-131) were built, tested and running, but the stop-report path never fed them: `HybridRepository::report_playback_stopped` is a bare pass-through to the online repository ("Playback reporting goes directly to server"), and on failure the error surfaced to a frontend `catch` whose own comment read "Server error - could queue, but for now just log". Both producers that *would* have queued it — `PlaybackReporter::queue_for_sync` in Rust and `syncService.queuePlaybackProgress` on the frontend — have no callers on the playback path, so closing a video while the server was unreachable lost the resume point outright even though `user_data.pending_sync` was dutifully set to 1 and nothing ever drains that flag for positions (unlike favourites, DR-120). The command layer now enqueues a `report_playback_stopped` row whenever the push fails, which the existing drain already knows how to parse and replay. The pending row for an item is **superseded in place** rather than appended to: progress is reported every 10s, so a server that stays down would otherwise add a row per tick, all of them obsoleted by the newest — the unbounded queue DR-131 exists to prevent. Only `pending`/`failed` rows are superseded, because an `abandoned` row has been given up on and reviving it would restore that same growing counter. Queueing is best-effort and never fails the command: the local position is already saved, so a failed *queue* write must not be reported as a lost position | Backend | UR-025, UR-002 | Done |
| DR-155 | A watch position set on another device reaches this one. The resume check reads the local `user_data` row and nothing else, but `mirror_user_data` — the only path by which server `UserData` lands in that table — mirrored `is_favorite` alone, and returned early whenever that field was absent, which is exactly the shape of an ordinary watched episode. So `playback_position_ticks` was write-only from this device's perspective: watch 40 minutes in a browser, open JellyTau, and it resumed from whatever *this* device last saw or offered no resume at all — the same user-visible symptom as DR-150's Android bug, from an unrelated cause, which is why resume read as broadly flaky. The mirror now carries the position alongside the favourite flag under the same `pending_sync = 0` conflict rule, so a local position still waiting to be pushed is never pulled *backwards* by a server that has not yet heard where we got to; `COALESCE(excluded.x, user_data.x)` means a field the server omitted keeps its stored value rather than being nulled, and a row with neither field is still skipped rather than fabricated as zeroes. Mirroring alone was not sufficient: `get_item` — the call the player route makes — returned the cached copy on a hit and never consulted the server, so for an already-cached item the mirror never ran. It now refreshes in the background on a cache hit (`race_with_refresh`, the reusable form of what `get_items` already did inline), which is why browsing a season picked up other devices' state while opening the episode directly did not. The refreshed value lands for the next read, the cache-first race still answering immediately | Backend | UR-025, UR-002 | Done |
| DR-143 | Flipping the offline downloaded-only gate actually re-queries the listing. The gate (DR-078) is a process-wide flag in Rust consulted only *while a query runs*, but no library surface re-queried when its inputs changed: `useServerReachabilityReload` fires only on the offline → **online** transition, and `GenericMediaListPage`, `GenericGenreBrowser` and the favourites page never even called its `checkServerReachability`. So going offline left the full server catalog on screen under a now-closed gate, and toggling "Show all server media" only greyed cards — `MediaCard.isServerOnly` is a pure frontend derivation that updates instantly — without adding or removing a single row. The filter therefore read as "shows everything until I filter, then greys some of it" while the backend gate was correct and simply never exercised. `catalogFilterVersion` is the refetch signal: `pushCatalogVisibility` now awaits `set_show_server_catalog` and bumps the version only **after** the backend accepts the new flag, since a reload racing the push would re-query under the old gate and undo itself. A failed push clears `lastIncludeCatalog` instead of latching it, so the next identical transition is retried rather than skipped as a no-op and left permanently disagreeing with the backend. `useOfflineFilterReload` subscribes pages to that signal, skipping the value they already loaded under; it is wired into both generic list components and the movies/music/tv/favourites landing pages and the `/library/[id]` detail page | UI | UR-052 | Done |
| DR-135 | A download's media type comes from the item, not a default. `download_item` — the path a media card uses to queue an item while offline — never records `media_type`, and the reconnect resolver read that NULL as `'audio'`, so a **movie** queued from a card had its URL resolved by `get_audio_stream_url`. The file that landed on disk was an audio-only transcode, which is why a "downloaded" film could never play offline no matter how the path or protocol was fixed. The resolver now falls back to the item's own `item_type` (`VIDEO_ITEM_TYPES` in Rust, so the frontend never learns which types are video) and only defaults to audio when the item is not cached locally. An explicit `media_type` on the row still wins | Downloads | UR-071, UR-052 | Done |
| DR-136 | Rows already downloaded under the audio default are repaired, not just prevented. They are identifiable after the fact — no `media_type`, but a video item — so on reconnect they are reset to `pending` with their audio URL cleared and re-resolved by DR-135's corrected logic, overwriting the audio file in place. Without this the fix is invisible to anyone who had already queued a film: the row still reads "downloaded" and still fails to play. Rows carrying an explicit `media_type` and genuine audio downloads are left untouched | Downloads | UR-071 | Done |
| DR-137 | Local media is served to the player over a loopback HTTP server, not the asset protocol. Tauri's `asset` protocol answers a request carrying no `Range` header by reading the whole file into memory, and only advertises `Accept-Ranges: bytes` from *inside* its range branch — so the first request never learns ranges exist and a multi-gigabyte body is attempted instead. Chromium abandoned it with `PIPELINE_ERROR_READ` after ~31s, which reached the user as "downloaded video does not play offline". Real HTTP on `127.0.0.1` is chosen over a custom URI scheme deliberately: range support becomes a property of the transport rather than depending on whether a platform's webview forwards `Range` to a custom scheme. No response ever exceeds a 4 MiB chunk and bodies stream from the file handle, so memory is bounded regardless of file size. Because **loopback is shared between apps on Android**, the server binds `127.0.0.1` only and every URL carries a random per-session token; paths are additionally confined to the app data directory, so a leaked URL cannot read outside it. This is stage 1 of making the server the single media origin — remote passthrough and download-while-watching are deliberately out of scope here | Playback | UR-071 | Done |
| DR-138 | Loopback is exempted from Android's cleartext ban, and nothing else is. Release builds set `usesCleartextTraffic="false"`, so the webview's request to the local media server (DR-137) was rejected by network security policy before any I/O — `<video>` failed in the same millisecond as `loadstart`, with `NETWORK_NO_SOURCE` and no server-side log at all, which is why it looked identical to a missing file. A `network-security-config` resource permits cleartext for `127.0.0.1` only and keeps `base-config cleartextTrafficPermitted="false"`, so a remote server must still be HTTPS; this is deliberately not a blanket opt-in. The manifest attribute is ignored once the config is present, so the config is the single authority. `sync-android-sources.sh` also had to learn to copy `res/xml`, which it skipped — the manifest references the resource, so a missed copy fails the resource link rather than degrading quietly | Security | UR-071 | Done |
| DR-093 | Traceability coverage gate derives its requirement denominators from `requirements.md` at run time rather than hardcoded literals: `countDefinedRequirements` counts an ID only where it leads a markdown table row (ignoring the "Traces To" column and prose) and deduplicates IDs listed both in the definition tables and in the §3 traceability matrix; `computeCoverage` reports the *intersection* of traced and defined IDs so an ID traced in code but absent from `requirements.md` is surfaced as `orphaned` instead of inflating the ratio past 100%. UT/IT test identifiers are excluded as a separate taxonomy. CI and `bun run traces:coverage` share this computation and fail on both a sub-threshold and an impossible >100% result | Tooling | - | Done |

---

## 3. Traceability Matrix

### User Requirements to Software Requirements

| User Req | Integration Requirements | Development Requirements |
|----------|-------------------------|-------------------------|
| UR-001 | IR-001, IR-002 | - |
| UR-002 | IR-013 | DR-003, DR-012, DR-013, DR-014 |
| UR-003 | IR-003, IR-004, IR-011 | DR-002, DR-004, DR-010 |
| UR-004 | IR-003, IR-004, IR-008, IR-011 | DR-002, DR-004, DR-006, DR-129 |
| UR-005 | - | DR-001, DR-005, DR-009 |
| UR-006 | IR-005, IR-006, IR-007, IR-008 | - |
| UR-007 | IR-010 | DR-007, DR-008, DR-016 |
| UR-008 | IR-010 | DR-007, DR-011 |
| UR-009 | IR-009, IR-010, IR-011 | - |
| UR-010 | IR-012, IR-021 | DR-037, DR-059 |
| UR-011 | IR-013 | DR-003, DR-015, DR-018 |
| UR-012 | IR-009, IR-014 | - |
| UR-013 | IR-013 | DR-017 |
| UR-014 | IR-010 | DR-014, DR-019 |
| UR-015 | - | DR-005, DR-020 |
| UR-016 | - | - |
| UR-017 | - | DR-014, DR-021 |
| UR-018 | IR-013 | DR-015, DR-018 |
| UR-019 | IR-015 | DR-022 |
| UR-020 | IR-016, IR-018 | DR-023 |
| UR-021 | IR-016, IR-019 | DR-024 |
| UR-022 | IR-017 | DR-025 |
| UR-023 | IR-010 | DR-026, DR-047, DR-048, DR-049 |
| UR-024 | IR-010 | DR-027 |
| UR-025 | IR-015 | DR-028, DR-131, DR-132 |
| UR-026 | - | DR-029, DR-048, DR-050 |
| UR-027 | IR-020 | DR-030 |
| UR-028 | - | DR-031 |
| UR-029 | - | DR-032 |
| UR-030 | IR-010 | DR-033 |
| UR-031 | - | DR-034 |
| UR-032 | - | DR-035 |
| UR-033 | - | DR-036 |
| UR-034 | IR-010, IR-024 | DR-038, DR-039 |
| UR-035 | IR-022, IR-023 | DR-040, DR-044 |
| UR-036 | IR-022, IR-023 | DR-041 |
| UR-037 | IR-010 | DR-042 |
| UR-038 | IR-010 | DR-043 |
| UR-039 | - | DR-045, DR-046 |
| UR-040 | IR-025 | DR-051, DR-052, DR-129, DR-130 |
| UR-041 | IR-026 | DR-053 |
| UR-042 | IR-009, IR-014 | DR-054 |
| UR-043 | IR-027 | DR-055 |
| UR-044 | - | DR-056 |
| UR-045 | - | DR-057 |
| UR-046 | IR-028 | DR-058 |
| UR-047 | IR-013 | DR-060 |
| UR-048 | - | DR-061, DR-062, DR-142 |
| UR-049 | IR-010 | DR-063, DR-064, DR-065, DR-147 |
| UR-050 | - | DR-066, DR-067 |
| UR-051 | - | DR-068, DR-069, DR-070 |
| UR-052 | IR-027 | DR-078, DR-079, DR-080, DR-143 |
| UR-053 | IR-029 | DR-074 |
| UR-054 | - | DR-075, DR-076, DR-077, DR-147 |
| UR-055 | - | DR-081, DR-082, DR-083, DR-084 |
| UR-056 | - | DR-085 |
| UR-057 | - | DR-086 |
| UR-058 | - | DR-087, DR-142 |
| UR-060 | - | DR-090, DR-091, DR-111 |
| UR-061 | - | DR-092 |
| UR-062 | - | DR-101, DR-102, DR-103, DR-104, DR-107 |
| UR-063 | - | DR-105 |
| UR-064 | - | DR-106 |
| UR-065 | IR-030 | DR-108, DR-109, DR-110, DR-111 |
| UR-066 | IR-031 | DR-112 |
| UR-067 | - | DR-115, DR-116, DR-117, DR-118 |
| UR-068 | - | DR-119 |
| UR-069 | - | DR-113, DR-114, DR-120 |
| UR-070 | - | DR-121, DR-122 |
| UR-071 | IR-032 | DR-123, DR-124, DR-125, DR-126, DR-127, DR-128, DR-133, DR-134, DR-135, DR-136, DR-137, DR-138 |

---

## 4. Test Traceability

### Unit Tests to Software Requirements

| Test ID | Test Description | Traces To | Status |
|---------|-----------------|-----------|--------|
| UT-001 | Player state transitions | DR-001 | Pending |
| UT-002 | MediaItem source URL resolution | DR-002, DR-003 | Pending |
| UT-003 | Queue next/previous navigation | DR-005 | Pending |
| UT-004 | Queue shuffle order generation | DR-005 | Pending |
| UT-005 | Queue repeat mode behavior | DR-005 | Pending |
| UT-006 | Jellyfin authentication flow | IR-009 | Pending |
| UT-007 | Jellyfin library items parsing | IR-010 | Pending |
| UT-008 | Repository pattern online/offline switching | DR-013 | Pending |
| UT-009 | Offline mutation queue persistence | DR-014 | Pending |
| UT-010 | Download queue management | DR-015 | Done |
| UT-011 | Resume position storage and retrieval | DR-022 | Pending |
| UT-012 | Sleep timer countdown logic | DR-029 | Pending |
| UT-013 | Playback progress reporting throttling | DR-028 | Pending |
| UT-014 | Database open and in-memory mode | IR-013, DR-012 | Done |
| UT-015 | Database migrations run successfully | IR-013, DR-012 | Done |
| UT-016 | All database tables created | IR-013, DR-012 | Done |
| UT-017 | FTS5 search table created | IR-013, DR-012 | Done |
| UT-018 | Server CRUD operations | IR-013, DR-012 | Done |
| UT-019 | User CRUD operations | IR-013, DR-012 | Done |
| UT-020 | Cascade delete server removes users | IR-013, DR-012 | Done |
| UT-021 | Item insert and FTS search | IR-013, DR-012 | Done |
| UT-022 | User data playback position storage | IR-013, DR-012, DR-022 | Done |
| UT-023 | Sync queue operations | IR-013, DR-014 | Done |
| UT-024 | Downloads table operations | IR-013, DR-015 | Done |
| UT-025 | Migrations are idempotent | IR-013, DR-012 | Done |
| UT-026 | NullBackend volume default value | DR-004 | Done |
| UT-027 | NullBackend set volume | DR-004 | Done |
| UT-028 | NullBackend volume clamping (high/low) | DR-004 | Done |
| UT-029 | NullBackend volume boundary values | DR-004 | Done |
| UT-030 | PlayerController volume default | DR-004, DR-009 | Done |
| UT-031 | PlayerController set volume | DR-004, DR-009 | Done |
| UT-032 | PlayerController muted default | DR-004, DR-009 | Done |
| UT-033 | PlayerController volume delegates to backend | DR-004, DR-009 | Done |
| UT-034 | Download event serialization roundtrip | DR-015 | Done |
| UT-035 | Download event completed serialization | DR-015 | Done |
| UT-036 | Download event failed serialization | DR-015 | Done |
| UT-037 | Download worker exponential backoff | DR-015 | Done |
| UT-038 | Download worker error retryable check | DR-015 | Done |
| UT-039 | Download manager creation | DR-015 | Done |
| UT-040 | Download manager set max concurrent | DR-015 | Done |
| UT-041 | Download info serialization | DR-015 | Done |
| UT-042 | Download command filename sanitization | DR-015, DR-018 | Done |
| UT-043 | Download command filename extension preservation | DR-015, DR-018 | Done |
| UT-044 | Offline item serialization | DR-017 | Done |
| UT-045 | Smart cache default config | DR-015 | Done |
| UT-046 | Smart cache album affinity tracking | DR-015 | Done |
| UT-047 | Smart cache queue precache config | DR-015 | Done |
| UT-048 | Smart cache storage limit check | DR-015 | Done |
| UT-049 | Playlist create (offline) | DR-019, JA-019 | Done |
| UT-050 | Playlist delete (offline) | DR-019, JA-019 | Done |
| UT-051 | Playlist rename (offline) | DR-019, JA-019 | Done |
| UT-052 | Playlist get items (offline) | DR-019, JA-019 | Done |
| UT-053 | Playlist add items (offline) | DR-019, JA-020 | Done |
| UT-054 | Playlist remove items (offline) | DR-019, JA-020 | Done |
| UT-055 | Playlist reorder items (offline) | DR-019, JA-020 | Done |
| UT-056 | Playlist entry serialization | DR-019, JA-019 | Done |
| UT-057 | Playlist Tauri command param naming (camelCase) | DR-019, JA-019, JA-020 | Done |
| UT-058 | Playlist repository client methods | DR-019, JA-019, JA-020 | Done |
| UT-059 | Audio-only stream URL builder for a video item (selected audio-stream index) | JA-032, DR-052 | Pending |
| UT-060 | Background-audio handoff state machine (background→audio, foreground→video; no dual audio) | DR-052 | Pending |
| UT-061 | Background-audio Tauri command param naming (camelCase) | DR-052 | Pending |
| UT-062 | `setBackgroundAudioEnabled` reports whether the native bridge was actually reached (missing bridge, stale proxy, throwing method) so a dead bridge cannot look armed | UR-040, IR-025, DR-051 | Done |
| UT-067 | Offline `get_items` gates the synced-catalog UNION on the catalog-browse flag (downloads only when off, full catalog when on) | DR-078 | Done |
| UT-068 | Catalog visibility resolves to `serverReachable \|\| showServerCatalog`, and is pushed to the backend on every change of either input | DR-078, DR-079 | Done |
| UT-069 | `isConnected` follows backend reachability alone: false when the server is unreachable on a live link, true for a reachable server while `navigator.onLine` is false | DR-079 | Done |
| UT-070 | Hybrid `get_items` returns an empty offline result as-is when the catalog-browse gate is off, without querying the server | DR-080 | Done |
| UT-066 | WiFi-only download gate: cellular and metered WiFi blocked, unmetered WiFi/Ethernet allowed, unknown/none fail closed, desktop default ungated; plus the frontend network reporter (transport reporting, change subscription, teardown, fail-open queries) | DR-074 | Done |
| UT-071 | Byte-size formatter: zero/negative/non-finite → "0 B"; decimal unit thresholds; 2–3 significant-figure banding; trailing-zero trimming; largest-unit cap | DR-085 | Done |
| UT-072 | Downloaded-only browse returns a downloaded leaf and its container, filtered to the requested album parent; a non-downloaded sibling is omitted | DR-082, DR-083 | Done |
| UT-073 | An empty downloaded-only browse is authoritative — no rows, no error — regardless of the catalog-browse flag | DR-082 | Done |
| UT-074 | Only libraries with downloaded content are listed; an empty one is omitted | DR-082 | Done |
| UT-075 | Disk usage reports a leaf's own size, a container's summed descendants, and reconciles the device total with the sum of leaves | DR-085 | Done |
| UT-076 | Downloaded library browse lists album containers, not their individual tracks; drilling into the album returns the tracks | DR-082, DR-083 | Done |
| UT-077 | Downloaded TV library browse lists the series, not seasons/episodes; drilling returns the season then the episode | DR-082, DR-083 | Done |
| UT-078 | A downloaded leaf with no cached container (e.g. a movie) still surfaces at the library level | DR-082, DR-083 | Done |
| UT-079 | Each EQ preset returns a 10-band gain curve within range; Flat is all zeros; Bass Boost lifts lows and leaves highs flat | DR-030 | Done |
| UT-080 | `with_equalizer_normalised` clamps out-of-range gains and forces the band vector to exactly 10 entries (pad short, truncate long) | DR-030 | Done |
| UT-081 | Old persisted AudioSettings JSON without EQ fields loads as disabled + flat | DR-030 | Done |
| UT-082 | EQ fields serialize as camelCase (`equalizerEnabled`/`equalizerBands`) and round-trip | DR-030 | Done |
| UT-083 | EQ filter entries are empty when disabled or when the curve is flat (clears the `af` filter) | IR-020 | Done |
| UT-084 | Enabled EQ builds one peaking `equalizer` per non-zero band at the right frequency and gain inside a single `lavfi` chain | IR-020 | Done |
| UT-085 | A first tap resolves to `togglePlayPause` immediately — no deferral and no timer | DR-092, DR-098 | Done |
| UT-086 | A second tap inside the window seeks (+30 s right half, −10 s left half) with the matching feedback side **and** re-toggles play/pause, so the two toggles cancel and the play state is unchanged by a double tap | DR-092, DR-098 | Done |
| UT-087 | A tap after the window, and the tap following a consumed pair, are each fresh first taps that toggle (there is no third-tap case); repeated double taps keep seeking; `cancel()` makes the next tap a first tap so an interpreted swipe cannot seek | DR-092, DR-098 | Done |
| UT-088 | `resolveSeekTarget` applies the delta to the reported position, clamps into `[0, duration - END_SEEK_MARGIN_SECONDS]`, chains off an in-flight pending target so rapid skips accumulate, and ignores that target once the player reports past it | DR-092, DR-095 | Done |
| UT-089 | A touch drag on the video seek bar seeks to the dragged position, never toggles play/pause, and never alters brightness — the container gesture layer stays out of a control drag entirely | DR-098, DR-099 | Done |
| UT-090 | The seek bar commits its seek on `touchend` even when the engine never fires `change`, and commits exactly once when both signals arrive | DR-099 | Done |
| UT-091 | Transport intents (play/pause/toggle) reach the backend even while a video adapter is registered, and never call the adapter's own `play`/`pause`/`toggle` — the webview must not decide play-vs-pause from the DOM | DR-097 | Done |
| UT-092 | `shouldReuseActivePlayback` reuses backend playback for an already-loaded audio track but never for video, and never when an explicit start position or a next-episode restart was requested | DR-100 | Done |
| UT-093 | `resolvePlayerSurface` returns `video` only with a stream URL, `pending` for video whose stream URL is still missing (never `audio`), and `audio` for audio content | DR-100 | Done |
| UT-094 | `parseNativeInsets` accepts the bridge's JSON or a decoded object, and coerces missing/negative/non-finite edges to 0 rather than emitting `NaNpx` (which would invalidate the whole padding declaration) | DR-112 | Done |
| UT-095 | `safeAreaCssVars`/`applySafeAreaInsets` emit px-suffixed `jt-inset` custom properties for all four edges | DR-112 | Done |
| UT-096 | `readNativeInsets` returns null with no bridge and survives a stale WebView proxy (missing or throwing `get`) instead of throwing out of layout init | IR-031, DR-112 | Done |
| UT-097 | `initSafeArea` primes the document on start, re-applies on `jellytau-insets-changed` (rotation, nav-mode switch), unsubscribes on teardown, and writes nothing without a bridge so `env()` still wins on iOS/desktop | IR-031, DR-112 | Done |
| UT-098 | `shellReservesBottomInset` gives the bottom inset to BottomUi wherever one renders and to the app shell only on routes without one, so the gesture bar is never ignored nor double-padded | DR-112 | Done |
| UT-099 | A Jellyfin item payload carrying `UserData.IsFavorite` maps to `MediaItem.user_data.is_favorite` | DR-113, JA-034 | Done |
| UT-100 | `OnlineRepository::get_favorites` builds `Filters=IsFavorite` + `Recursive=true` + the scope's `IncludeItemTypes`, and omits the type filter entirely for `SearchScope::All` | DR-115, JA-033 | Done |
| UT-101 | `OfflineRepository::get_favorites` returns only `is_favorite = 1` rows, honours the scope type filter, and stays downloads-only when the catalog-browse gate is off | DR-115 | Done |
| UT-102 | The `save_to_cache` favourite mirror does not overwrite a row with `pending_sync = 1` | DR-114 | Done |
| UT-103 | The reconnect drain pushes pending favourites, clears `pending_sync`, and leaves failed rows pending | DR-120 | Done |
| UT-104 | `get_items` with `favorites_only` filters online (endpoint) and offline (SQL) | DR-116 | Done |
| UT-105 | `favorites` store precedence: override beats `userData.isFavorite` beats `false` | DR-119 | Done |
| UT-106 | Un-favouriting removes an item from a favourites listing view | DR-117, DR-119 | Done |
| UT-107 | The hybrid background refresh emits `favorites-changed` only for ids whose favourite state actually flipped | DR-120 | Done |
| UT-109 | Search covers synced-but-not-downloaded items when catalog browse is on, and stays downloads-only when off | DR-108 | Done |
| UT-110 | Search item-type filter is bound, not interpolated: a quote-bearing type neither errors nor widens results | DR-108 | Done |
| UT-111 | FTS prefix queries quote each token, so apostrophes/hyphens/slashes are data; empty or punctuation-only input returns no rows rather than erroring | DR-108 | Done |
| UT-112 | Repeated catalog passes leave one `items_fts` entry per item, not one per pass | DR-110 | Done |
| UT-113 | The stale-catalog sweep removes vanished synced rows, keeps downloaded ones, keeps uncrawled types, and stays scoped to one server | DR-110 | Done |
| UT-114 | Cached people are reachable from unscoped search and excluded from scoped search | DR-111 | Done |
| UT-115 | Re-index staleness policy: never-indexed and unparseable timestamps are due, fresh ones are not, future ones are not | DR-109 | Done |
| UT-116 | `resolve_local_media_path` returns a completed download's file, and `None` for an in-progress download, a row whose file has been deleted, or an unknown item | DR-123 | Done |
| UT-118 | `resolveVideoSource` prefers a downloaded file, never marks a local file as needing transcoding, and falls back to streaming for a blank path | DR-123 | Done |
| UT-119 | The audio-only handoff picks a downloaded file over the audio-only stream URL, preserving the Jellyfin id for progress sync | DR-128 | Done |
| UT-120 | Expiry reclaim takes only expired temporary entries: derived from `completed_at`+TTL, honouring an `expires_at` override, never a user download, and disabled by a zero TTL | DR-127 | Done |
| UT-108 | LRU eviction reclaims only `'auto'` downloads and never a user's own, even when the user's is the oldest | DR-126 | Done |
| UT-117 | A background audio-only stream cut short resumes where it died instead of ending the episode; a real end still advances; the absolute position is compared against the runtime; retries at a stuck position give up. A recoverable error resumes music and video too, with growing backoff, leaving the rest of the queue intact and the seekable stream's URL untouched; local and DirectUrl sources are excluded | DR-129 | Done |
| UT-124 | `downloadedFilePath` leaves a completed download's absolute path alone (POSIX and Windows) and only roots one that is still relative | DR-133 | Done |
| UT-125 | A NULL `media_type` resolves from the item type — Movie and Episode as video, a track as audio — an uncached item still defaults to audio, and an explicit `media_type` overrides the item | DR-135 | Done |
| UT-126 | Requeueing takes only video rows downloaded under the audio default, clearing their URL, and leaves correctly-typed video rows and real audio downloads alone | DR-136 | Done |
| UT-127 | The media server bounds and confines every response: a range-less request yields one chunk rather than the whole file, no range exceeds the chunk cap, explicit/open-ended/suffix ranges resolve correctly, a range past the end is unsatisfiable rather than clamped, a malformed header falls back to the first chunk, path traversal and unrelated absolute paths are refused, a wrong or absent token is rejected, and content type comes from the extension then the magic bytes | DR-137 | Done |
| UT-121 | An EOF reads as the last observed timestamp, not zero: live readings win while the file is loaded, a not-yet-established duration is not recorded as a real zero, a seek updates the position before the next poll, and loading a new file clears the previous one's | DR-130 | Done |
| UT-122 | The sync-queue drain pushes queued playback reports oldest-first, defers failures for the next reconnect, abandons a row after `MAX_SYNC_ATTEMPTS`, ignores other users' rows, and parses both payload dialects | DR-131 | Done |
| UT-123 | Pending-sync rows describe themselves: every queueable operation has a label, an unknown one still renders, the item title falls back to its id, and rows list oldest-first | DR-132 | Done |
| UT-130 | Video and background-audio stream URLs omit `AudioStreamIndex` when no track was chosen, and carry the exact index when one was | DR-140 | Done |
| UT-131 | The Episode Focus View hero offers a download control | DR-142 | Done |
| UT-132 | The series name links to the series and the `SxEy` badge to that season's anchor | DR-142 | Done |
| UT-133 | Cast renders below the "More Episodes" strip, never above it | DR-062, DR-142 | Done |
| UT-134 | The episode strip is hidden when the episode has no siblings | DR-142 | Done |
| UT-135 | An episode with no `seriesId` still renders the Focus View, with title, Play and download | DR-142 | Done |
| UT-136 | `episodeRedirectTarget` sends a bare episode page into its series' Focus View, and returns null with no series | DR-142 | Done |
| UT-137 | Going offline with the toggle off pushes the closed gate and bumps `catalogFilterVersion` | DR-143 | Done |
| UT-138 | The version bumps only after `set_show_server_catalog` resolves, never before | DR-143 | Done |
| UT-139 | A failed visibility push is retried on the next identical transition rather than latched | DR-143 | Done |
| UT-140 | `useOfflineFilterReload` skips the value a page already loaded under and reloads on each later change | DR-143 | Done |
| UT-141 | The advertised channel cap: an unknown or zero reading falls back to stereo, a real route keeps its channels, an absurd driver reading is capped at 7.1, and mono is taken at its word | DR-141 | Done |
| UT-148 | Forcing a transcode from the client: an undecodable default track forces one, a decodable track does not, the default track decides rather than the first, the first decides when nothing is marked default, and neither an audio-less source nor an unnamed codec is second-guessed | DR-149 | Done |
| UT-149 | `createAdapter` returns the native adapter only when Rust reports native AND `experimentalNativeVideo` is on; the flag off forces HTML5 even when Rust says native, and the flag on never promotes a platform Rust reported as HTML5 | DR-150 | Done |
| UT-150 | `set-version.sh` stamps all four manifests without touching dependency versions, and the Android versionCode is monotonic across an upgrade sequence, clears the 1000 floor, and survives a prerelease suffix | DR-153 | Done |
| UT-151 | An unreportable stop lands in the queue and is pushed by the existing drain; re-queueing the same item supersedes the earlier position rather than adding a row, distinct items keep their own positions, and an abandoned row is not revived by a later report | DR-154 | Done |
| UT-152 | Caching a server result mirrors its watch position locally — including for an item carrying a position but no favourite flag — without inventing a row for an item the server reported no user data for, and without pulling a still-unsynced local position backwards | DR-155 | Done |
| UT-142 | The audio codecs offered for video direct play: a Dolby device's real `MediaCodecList` output drops `ac3`/`eac3`, AMR and raw PCM are dropped too, a fully-supported list is passed through untouched, a list with nothing decodable still claims `aac`, and stray spacing or casing does not decide whether the user gets sound | DR-148 | Done |
| UT-143 | Subtitle URLs resolve to plain strings before they reach the markup (never a Promise), unresolvable tracks are dropped, a stale selection collapses to "Off", and a server-default track is never auto-selected | UR-020, DR-023 | Done |
| UT-144 | VideoPlayer actually renders `<track kind="subtitles">` children carrying `data-stream-index`, with no `default` attribute and no async `getSubtitleUrl()` bound to `src` | UR-020, DR-023 | Done |
| UT-145 | The frontend's subtitle payload survives the IPC hop: a camelCase `PlayItemRequest` carrying `subtitles` deserializes, `create_media_item` lands them on `MediaItem.subtitles` in the order sent, and a request without the field still defaults to empty | UR-020, IR-016 | Done |
| UT-146 | The subtitle JSON serialized across the JNI boundary uses the keys `JellyTauPlayer.load()` reads — `url`, `language`, `label` and `mime_type`, never `mimeType` | UR-020, IR-016, JA-008 | Done |
| UT-147 | The native subtitle payload and the track-selection index come from the same resolved list: the wire shape keeps `mime_type` and stream order, `playerPlayItem` actually sends it, and the index is a position in the sent list (so a track whose URL failed to resolve cannot shift the others) rather than the menu's row number | UR-020, IR-016 | Done |

### Integration Tests

| Test ID | Test Description | Traces To | Status |
|---------|-----------------|-----------|--------|
| IT-001 | End-to-end authentication with Jellyfin server | IR-009, UR-009 | Pending |
| IT-002 | Library browsing and item loading | IR-010, UR-007 | Pending |
| IT-003 | Audio playback via libmpv | IR-003, UR-004 | Pending |
| IT-004 | Video playback via libmpv | IR-003, UR-003 | Pending |
| IT-005 | MPRIS lockscreen controls on Linux | IR-005, UR-006 | Pending |
| IT-006 | Offline mode with local database | IR-013, UR-002 | Pending |
| IT-007 | Media download and local playback | DR-015, UR-011 | Pending |
| IT-008 | Subtitle track selection via libmpv | IR-018, UR-020 | Pending |
| IT-009 | Audio track selection via libmpv | IR-019, UR-021 | Pending |
| IT-010 | Playback progress sync to Jellyfin | IR-015, UR-025 | Pending |
| IT-011 | Resume playback from server position | IR-015, UR-019 | Pending |
| IT-012 | Equalizer bands via libmpv | IR-020, UR-027 | Pending |
| IT-013 | Background-audio handoff on Android: background/lock continues audio via native service and stops video decode; foreground resumes video at position | IR-025, UR-040 | Pending |
| IT-016 | Offline library listing end-to-end: with the server unreachable, a library page lists only downloaded media with the toggle off, and additionally reveals greyed-out cached catalog entries with the toggle on | UR-052, DR-078, DR-079, DR-080 | Done |
| IT-017 | A download queued from a greyed-out offline catalog entry persists and is resolved and started on reconnect | UR-052, UR-011 | Done |

---

## 5. Technical Debt

### Linux Keyring Integration Workaround

**Issue**: The `keyring-rs` crate (v3.x) has issues with retrieving credentials from the Linux Secret Service API, despite successfully saving them.

**Symptoms**:
- Credentials are saved to the system keyring successfully (verified with `secret-tool search`)
- Retrieval via the `keyring-rs` library fails with `NoEntry` error
- Session restoration fails on app restart even though credentials exist

**Root Cause**:
The `keyring-rs` library's Linux backend doesn't correctly retrieve entries from the Secret Service that it previously stored. This appears to be a bug in how the library interfaces with the Secret Service D-Bus API.

**Current Workaround**:
We bypass the `keyring-rs` library on Linux and use direct system calls to `secret-tool`:
- **Save**: `secret-tool store --label <label> service <service> username <username>`
- **Retrieve**: `secret-tool lookup service <service> username <username>`
- **Delete**: `secret-tool clear service <service> username <username>`

**Implementation**:
See [src-tauri/src/credentials.rs](../src-tauri/src/credentials.rs) for the
Linux-specific `secret-tool` save/get/delete paths.

**Future Fix**:
- Monitor `keyring-rs` for bug fixes in future versions
- Consider alternative secure storage libraries
- Test if newer versions of `keyring-rs` (v4.x+) resolve the issue
- Once fixed, remove the Linux-specific workaround and use the cross-platform `keyring-rs` API

**Impact**:
- Low - The workaround is functionally equivalent to proper keyring integration
- Credentials are stored securely in the system keyring
- Session restoration works correctly
- Only affects Linux; macOS and Windows use the standard `keyring-rs` implementation

**Dependencies**:
- Requires `secret-tool` to be installed on Linux systems (part of `libsecret-tools` package)
- Already available on most Linux distributions by default

---

### Platform Playback Backend Parity (Linux vs Android)

**Issue**: The Linux (MPV) and Android (ExoPlayer) playback backends have diverged in feature implementation and architecture patterns.

**Symptoms**:
- Audio settings (crossfade, gapless playback, volume normalization) work on Linux but not on Android
- Position update frequency differs between platforms (Linux: 250ms polling, Android: on-demand callbacks)
- Thread safety models differ (Linux: `Arc<Mutex<>>`, Android: global `OnceLock` statics)

**Root Cause**:
The `PlayerBackend` trait defines optional audio settings methods with default empty implementations. The Linux `MpvBackend` overrides these with full MPV property commands, but `ExoPlayerBackend` uses the defaults.

**Affected Files**:
- [src-tauri/src/player/backend.rs](../src-tauri/src/player/backend.rs) - Trait with default empty implementations
- [src-tauri/src/player/mpv_backend.rs](../src-tauri/src/player/mpv_backend.rs) - Full audio settings support
- [src-tauri/src/player/android/mod.rs](../src-tauri/src/player/android/mod.rs) - Missing audio settings implementation

**Feature Parity Matrix**:

| Feature | Linux (MPV) | Android (ExoPlayer) | Status |
|---------|-------------|---------------------|--------|
| Basic playback | ✅ | ✅ | Parity |
| Volume control | ✅ | ✅ | Parity |
| Seek | ✅ | ✅ | Parity |
| Crossfade | ❌ | ❌ | Not implemented (blocked on MPV) |
| Gapless playback | ✅ | ⚠️ | Implemented, pending on-device verification |
| Volume normalization | ✅ | ⚠️ | Implemented (LoudnessEnhancer — gain stage, approximate vs MPV's dynaudnorm), pending on-device verification |
| Equalizer (10-band) | ✅ | ⚠️ | Implemented (resampled onto device bands), pending on-device verification |
| Position updates | 250ms | On-demand | Inconsistent |

**Status** (see docs/specs/android-audio-settings-parity.md):
1. ✅ `set_audio_settings()` implemented in `ExoPlayerBackend` (JSON over JNI)
2. ✅ Gapless via ExoPlayer's `pauseAtEndOfMediaItems`
3. ✅ Volume normalization via `LoudnessEnhancer`
4. ✅ Equalizer via `android.media.audiofx.Equalizer`, canonical 10 bands
   resampled onto the device's band centres
5. ⬜ **Not yet verified on a physical device** — the EQ/normalization effects
   depend on device-specific `AudioEffect` availability and band layouts
6. ⬜ Flip the trait's `set_audio_settings` default from `Ok(())` to
   `Err(not_implemented())` so a backend that omits it fails loudly instead of
   silently reporting success. Deferred until (5) confirms the Android path works
7. ⬜ Standardize position update frequency across platforms

Crossfade is deliberately absent: it is unimplemented on every platform and
architecturally blocked on MPV, so building it on Android alone would invert the
parity gap. (The previously suggested `ConcatenatingMediaSource` is also
deprecated in current Media3.)

**Impact**:
- Medium - Android users lack audio enhancement features advertised in requirements
- User experience differs between platforms
- UR-032 (Gapless), UR-033 (Normalization) and UR-027 (Equalizer) are now
  implemented on Android as well as Linux, pending on-device verification
- UR-031 (Crossfade) works nowhere — see DR-034

**Traces To**: IR-004, UR-031, UR-032, UR-033, DR-034, DR-035, DR-036

---

### Frontend Playback Code Duplication

**Issue**: Playback control handlers and state derivations are duplicated between `AudioPlayer.svelte` and `MiniPlayer.svelte`.

**Symptoms**:
- Identical try-catch wrapped handler functions in both components (~44 lines duplicated)
- Same `$derived` state merging logic for local/remote playback in both components
- Position conversion (ticks ↔ seconds) scattered across multiple files

**Affected Files**:
- [src/lib/components/player/AudioPlayer.svelte](../src/lib/components/player/AudioPlayer.svelte) - Duplicate handlers
- [src/lib/components/player/MiniPlayer.svelte](../src/lib/components/player/MiniPlayer.svelte) - Duplicate handlers
- [src/lib/services/playbackControl.ts](../src/lib/services/playbackControl.ts) - Position conversion
- [src/lib/stores/playbackMode.ts](../src/lib/stores/playbackMode.ts) - Position conversion
- [src/lib/services/playbackReporting.ts](../src/lib/services/playbackReporting.ts) - Position conversion

**Duplicated Code**:
```typescript
// These handlers are identical in both AudioPlayer and MiniPlayer:
handlePlayPause(), handleNext(), handlePrevious(),
handleToggleShuffle(), handleCycleRepeat(), handleVolumeChange()

// These derived states use identical logic:
displayMedia, displayIsPlaying, displayPosition, displayDuration
```

**Future Fix**:
1. Create `src/lib/utils/playbackUnits.ts`:
   ```typescript
   export const TICKS_PER_SECOND = 10_000_000;
   export const secondsToTicks = (s: number) => Math.floor(s * TICKS_PER_SECOND);
   export const ticksToSeconds = (t: number) => t / TICKS_PER_SECOND;
   ```

2. Create `src/lib/composables/useMergedPlaybackState.svelte.ts`:
   - Export `displayMedia`, `displayIsPlaying`, `displayPosition`, `displayDuration`
   - Single source of truth for merged local/remote state

3. Simplify handler wrappers using a utility:
   ```typescript
   export const withErrorHandler = (fn: () => Promise<void>, context: string) =>
     async () => { try { await fn(); } catch (e) { console.error(`${context}:`, e); } };
   ```

**Impact**:
- Low - Code works correctly but violates DRY principle
- Maintenance burden when logic needs to change
- Risk of handlers diverging over time

**Traces To**: DR-009
